———————————————————————————
LTE  2600
———————————————————————————

MASTER INFORMATION BLOCK
LTE MIB Message
  Version : 2
  Physical Cell ID : 459
  E-ARFCN : 37950
  SFN : 432
  Num TX Antennas : 2
  DL Bandwidth : 20 MHz (100)

SYSTEM INFORMATION BLOCK TYPE 1
LTE RRC Signaling Messages
  Version : 15
  RRC Release Number : 13
  RRC Version Minor : 1
  RRC Version Major : 2
  RB ID : 0
  Physical Cell ID : 459
  E-ARFCN : 37950
  SFN : 23333
  Channel : 2
  Bitmask of SIBS : 2
  Message Length : 28
  bcch-dl-sch
    message
      c1
        systemInformationBlockType1
          cellAccessRelatedInfo
            plmn-IdentityList
              PLMN-IdentityList[0]
                plmn-Identity
                  mcc
                    MCC[0]
                      MCC-MNC-Digit : 2
                    MCC[1]
                      MCC-MNC-Digit : 2
                    MCC[2]
                      MCC-MNC-Digit : 6
                  mnc
                    MNC[0]
                      MCC-MNC-Digit : 0
                    MNC[1]
                      MCC-MNC-Digit : 5
                cellReservedForOperatorUse : notReserved
            trackingAreaCode : 02BC(16 bits)
            cellIdentity : 186E90B0(28 bits)
            cellBarred : notBarred
            intraFreqReselection : allowed
            csg-Indication : false
          cellSelectionInfo
            q-RxLevMin : -64
          freqBandIndicator : 38
          schedulingInfoList
            SchedulingInfoList[0]
              si-Periodicity : rf8
              sib-MappingInfo
                SIB-MappingInfo[0]
                  SIB-Type : sibType3
            SchedulingInfoList[1]
              si-Periodicity : rf64
              sib-MappingInfo
                SIB-MappingInfo[0]
                  SIB-Type : sibType4
            SchedulingInfoList[2]
              si-Periodicity : rf64
              sib-MappingInfo
                SIB-MappingInfo[0]
                  SIB-Type : sibType5
            SchedulingInfoList[3]
              si-Periodicity : rf64
              sib-MappingInfo
                SIB-MappingInfo[0]
                  SIB-Type : sibType6
          tdd-Config
            subframeAssignment : sa2
            specialSubframePatterns : ssp7
          si-WindowLength : ms10
          systemInfoValueTag : 30
          nonCriticalExtension
            lateNonCriticalExtension
              multiBandInfoList
                MultiBandInfoList[0]
                  FreqBandIndicator : 41

SYSTEM INFORMATION
LTE RRC Signaling Messages
  Version : 15
  RRC Release Number : 13
  RRC Version Minor : 1
  RRC Version Major : 2
  RB ID : 0
  Physical Cell ID : 459
  E-ARFCN : 37950
  SFN : 0
  Channel : 2
  Bitmask of SIBS : 12
  Message Length : 47
  bcch-dl-sch
    message
      c1
        systemInformation
          criticalExtensions
            systemInformation-r8
              sib-TypeAndInfo[0]
                sib2
                  radioResourceConfigCommon
                    rach-ConfigCommon
                      preambleInfo
                        numberOfRA-Preambles : n52
                      powerRampingParameters
                        powerRampingStep : dB4
                        preambleInitialReceivedTargetPower : dBm-110
                      ra-SupervisionInfo
                        preambleTransMax : n10
                        ra-ResponseWindowSize : sf10
                        mac-ContentionResolutionTimer : sf64
                      maxHARQ-Msg3Tx : 4
                    bcch-Config
                      modificationPeriodCoeff : n2
                    pcch-Config
                      defaultPagingCycle : rf128
                      nB : oneT
                    prach-Config
                      rootSequenceIndex : 763
                      prach-ConfigInfo
                        prach-ConfigIndex : 3
                        highSpeedFlag : false
                        zeroCorrelationZoneConfig : 12
                        prach-FreqOffset : 7
                    pdsch-ConfigCommon
                      referenceSignalPower : 15
                      p-b : 0
                    pusch-ConfigCommon
                      pusch-ConfigBasic
                        n-SB : 1
                        hoppingMode : interSubFrame
                        pusch-HoppingOffset : 0
                        enable64QAM : true
                      ul-ReferenceSignalsPUSCH
                        groupHoppingEnabled : true
                        groupAssignmentPUSCH : 0
                        sequenceHoppingEnabled : false
                        cyclicShift : 0
                    pucch-ConfigCommon
                      deltaPUCCH-Shift : ds1
                      nRB-CQI : 5
                      nCS-AN : 0
                      n1PUCCH-AN : 80
                    soundingRS-UL-ConfigCommon
                    uplinkPowerControlCommon
                      p0-NominalPUSCH : -103
                      alpha : al1
                      p0-NominalPUCCH : -117
                      deltaFList-PUCCH
                        deltaF-PUCCH-Format1 : deltaF0
                        deltaF-PUCCH-Format1b : deltaF3
                        deltaF-PUCCH-Format2 : deltaF0
                        deltaF-PUCCH-Format2a : deltaF0
                        deltaF-PUCCH-Format2b : deltaF0
                      deltaPreambleMsg3 : 6
                    ul-CyclicPrefixLength : len1
                    pusch-ConfigCommon-v1270
                      enable64QAM-v1270 : true
                  ue-TimersAndConstants
                    t300 : ms1000
                    t301 : ms2000
                    t310 : ms2000
                    n310 : n20
                    t311 : ms5000
                    n311 : n1
                  freqInfo
                    additionalSpectrumEmission : 1
                  timeAlignmentTimerCommon : infinity
                  lateNonCriticalExtension
                    multiBandInfoList[0]
                      AdditionalSpectrumEmission : 1
              sib-TypeAndInfo[1]
                sib3
                  cellReselectionInfoCommon
                    q-Hyst : dB4
                  cellReselectionServingFreqInfo
                    s-NonIntraSearch : 6
                    threshServingLow : 5
                    cellReselectionPriority : 7
                  intraFreqCellReselectionInfo
                    q-RxLevMin : -64
                    allowedMeasBandwidth : mbw100
                    presenceAntennaPort1 : false
                    neighCellConfig : 80(2 bits)
                    t-ReselectionEUTRA : 2
                  s-IntraSearch-v920
                    s-IntraSearchP-r9 : 31
                    s-IntraSearchQ-r9 : 0
                  s-NonIntraSearch-v920
                    s-NonIntraSearchP-r9 : 6
                    s-NonIntraSearchQ-r9 : 0

SYSTEM INFORMATION
LTE RRC Signaling Messages
  Version : 15
  RRC Release Number : 13
  RRC Version Minor : 1
  RRC Version Major : 2
  RB ID : 0
  Physical Cell ID : 459
  E-ARFCN : 37950
  SFN : 0
  Channel : 2
  Bitmask of SIBS : 32
  Message Length : 32
  bcch-dl-sch
    message
      c1
        systemInformation
          criticalExtensions
            systemInformation-r8
              sib-TypeAndInfo[0]
                sib5
                  interFreqCarrierFreqList
                    InterFreqCarrierFreqList[0]
                      dl-CarrierFreq : 128
                      q-RxLevMin : -64
                      t-ReselectionEUTRA : 2
                      threshX-High : 2
                      threshX-Low : 8
                      allowedMeasBandwidth : mbw25
                      presenceAntennaPort1 : false
                      cellReselectionPriority : 6
                      neighCellConfig : 80(2 bits)
                    InterFreqCarrierFreqList[1]
                      dl-CarrierFreq : 103
                      q-RxLevMin : -64
                      t-ReselectionEUTRA : 2
                      threshX-High : 2
                      threshX-Low : 7
                      allowedMeasBandwidth : mbw50
                      presenceAntennaPort1 : false
                      cellReselectionPriority : 6
                      neighCellConfig : 80(2 bits)
                      interFreqNeighCellList
                        InterFreqNeighCellList[0]
                          physCellId : 365
                          q-OffsetCell : dB-1
                  lateNonCriticalExtension
                    interFreqCarrierFreqList-v8h0[0]
                      multiBandInfoList
                        MultiBandInfoList[0]
                          FreqBandIndicator : 64
                    interFreqCarrierFreqList-v8h0[1]
                      multiBandInfoList
                        MultiBandInfoList[0]
                          FreqBandIndicator : 64
                    nonCriticalExtension
                      interFreqCarrierFreqList-v9e0[0]
                        multiBandInfoList-v9e0
                          MultiBandInfoList-v9e0[0]
                            freqBandIndicator-v9e0 : 65
                      interFreqCarrierFreqList-v9e0[1]
                        multiBandInfoList-v9e0
                          MultiBandInfoList-v9e0[0]
                            freqBandIndicator-v9e0 : 65

SYSTEM INFORMATION
LTE RRC Signaling Messages
  Version : 15
  RRC Release Number : 13
  RRC Version Minor : 1
  RRC Version Major : 2
  RB ID : 0
  Physical Cell ID : 459
  E-ARFCN : 37950
  SFN : 0
  Channel : 2
  Bitmask of SIBS : 16
  Message Length : 7
  bcch-dl-sch
    message
      c1
        systemInformation
          criticalExtensions
            systemInformation-r8
              sib-TypeAndInfo[0]
                sib4
                  intraFreqNeighCellList
                    IntraFreqNeighCellList[0]
                      physCellId : 461
                      q-OffsetCell : dB3
                    IntraFreqNeighCellList[1]
                      physCellId : 460
                      q-OffsetCell : dB1

SYSTEM INFORMATION
LTE RRC Signaling Messages
  Version : 15
  RRC Release Number : 13
  RRC Version Minor : 1
  RRC Version Major : 2
  RB ID : 0
  Physical Cell ID : 459
  E-ARFCN : 37950
  SFN : 0
  Channel : 2
  Bitmask of SIBS : 64
  Message Length : 15
  bcch-dl-sch
    message
      c1
        systemInformation
          criticalExtensions
            systemInformation-r8
              sib-TypeAndInfo[0]
                sib6
                  carrierFreqListUTRA-FDD
                    CarrierFreqListUTRA-FDD[0]
                      carrierFreq : 10564
                      cellReselectionPriority : 4
                      threshX-High : 2
                      threshX-Low : 1
                      q-RxLevMin : -58
                      p-MaxUTRA : 33
                      q-QualMin : -18
                    CarrierFreqListUTRA-FDD[1]
                      carrierFreq : 2988
                      cellReselectionPriority : 4
                      threshX-High : 2
                      threshX-Low : 1
                      q-RxLevMin : -58
                      p-MaxUTRA : 33
                      q-QualMin : -18
                  t-ReselectionUTRA : 2

———————————————————————————
LTE 2100
———————————————————————————

MASTER INFORMATION BLOCK
LTE MIB Message
  Version : 2
  Physical Cell ID : 365
  E-ARFCN : 103
  SFN : 968
  Num TX Antennas : 2
  DL Bandwidth : 10 MHz (50)

SYSTEM INFORMATION BLOCK TYPE 1
LTE RRC Signaling Messages
  Version : 15
  RRC Release Number : 13
  RRC Version Minor : 1
  RRC Version Major : 2
  RB ID : 0
  Physical Cell ID : 365
  E-ARFCN : 103
  SFN : 31909
  Channel : 2
  Bitmask of SIBS : 2
  Message Length : 28
  bcch-dl-sch
    message
      c1
        systemInformationBlockType1
          cellAccessRelatedInfo
            plmn-IdentityList
              PLMN-IdentityList[0]
                plmn-Identity
                  mcc
                    MCC[0]
                      MCC-MNC-Digit : 2
                    MCC[1]
                      MCC-MNC-Digit : 2
                    MCC[2]
                      MCC-MNC-Digit : 6
                  mnc
                    MNC[0]
                      MCC-MNC-Digit : 0
                    MNC[1]
                      MCC-MNC-Digit : 5
                cellReservedForOperatorUse : notReserved
            trackingAreaCode : 02BC(16 bits)
            cellIdentity : 186E9150(28 bits)
            cellBarred : notBarred
            intraFreqReselection : allowed
            csg-Indication : false
          cellSelectionInfo
            q-RxLevMin : -64
          freqBandIndicator : 1
          schedulingInfoList
            SchedulingInfoList[0]
              si-Periodicity : rf8
              sib-MappingInfo
                SIB-MappingInfo[0]
                  SIB-Type : sibType3
            SchedulingInfoList[1]
              si-Periodicity : rf64
              sib-MappingInfo
                SIB-MappingInfo[0]
                  SIB-Type : sibType5
            SchedulingInfoList[2]
              si-Periodicity : rf64
              sib-MappingInfo
                SIB-MappingInfo[0]
                  SIB-Type : sibType6
          si-WindowLength : ms10
          systemInfoValueTag : 31
          nonCriticalExtension
            lateNonCriticalExtension
              multiBandInfoList
                MultiBandInfoList[0]
                  FreqBandIndicator : 64
              nonCriticalExtension
                multiBandInfoList-v9e0
                  MultiBandInfoList-v9e0[0]
                    freqBandIndicator-v9e0 : 65

SYSTEM INFORMATION
LTE RRC Signaling Messages
  Version : 15
  RRC Release Number : 13
  RRC Version Minor : 1
  RRC Version Major : 2
  RB ID : 0
  Physical Cell ID : 365
  E-ARFCN : 103
  SFN : 0
  Channel : 2
  Bitmask of SIBS : 12
  Message Length : 47
  bcch-dl-sch
    message
      c1
        systemInformation
          criticalExtensions
            systemInformation-r8
              sib-TypeAndInfo[0]
                sib2
                  radioResourceConfigCommon
                    rach-ConfigCommon
                      preambleInfo
                        numberOfRA-Preambles : n52
                      powerRampingParameters
                        powerRampingStep : dB4
                        preambleInitialReceivedTargetPower : dBm-110
                      ra-SupervisionInfo
                        preambleTransMax : n10
                        ra-ResponseWindowSize : sf10
                        mac-ContentionResolutionTimer : sf64
                      maxHARQ-Msg3Tx : 4
                    bcch-Config
                      modificationPeriodCoeff : n2
                    pcch-Config
                      defaultPagingCycle : rf128
                      nB : oneT
                    prach-Config
                      rootSequenceIndex : 633
                      prach-ConfigInfo
                        prach-ConfigIndex : 3
                        highSpeedFlag : false
                        zeroCorrelationZoneConfig : 12
                        prach-FreqOffset : 2
                    pdsch-ConfigCommon
                      referenceSignalPower : 20
                      p-b : 1
                    pusch-ConfigCommon
                      pusch-ConfigBasic
                        n-SB : 1
                        hoppingMode : interSubFrame
                        pusch-HoppingOffset : 0
                        enable64QAM : true
                      ul-ReferenceSignalsPUSCH
                        groupHoppingEnabled : true
                        groupAssignmentPUSCH : 0
                        sequenceHoppingEnabled : false
                        cyclicShift : 0
                    pucch-ConfigCommon
                      deltaPUCCH-Shift : ds1
                      nRB-CQI : 1
                      nCS-AN : 0
                      n1PUCCH-AN : 16
                    soundingRS-UL-ConfigCommon
                    uplinkPowerControlCommon
                      p0-NominalPUSCH : -103
                      alpha : al1
                      p0-NominalPUCCH : -117
                      deltaFList-PUCCH
                        deltaF-PUCCH-Format1 : deltaF0
                        deltaF-PUCCH-Format1b : deltaF3
                        deltaF-PUCCH-Format2 : deltaF0
                        deltaF-PUCCH-Format2a : deltaF0
                        deltaF-PUCCH-Format2b : deltaF0
                      deltaPreambleMsg3 : 6
                    ul-CyclicPrefixLength : len1
                    pusch-ConfigCommon-v1270
                      enable64QAM-v1270 : true
                  ue-TimersAndConstants
                    t300 : ms1000
                    t301 : ms2000
                    t310 : ms2000
                    n310 : n20
                    t311 : ms5000
                    n311 : n1
                  freqInfo
                    additionalSpectrumEmission : 1
                  timeAlignmentTimerCommon : infinity
                  lateNonCriticalExtension
                    multiBandInfoList[0]
                      AdditionalSpectrumEmission : 1
              sib-TypeAndInfo[1]
                sib3
                  cellReselectionInfoCommon
                    q-Hyst : dB4
                  cellReselectionServingFreqInfo
                    s-NonIntraSearch : 8
                    threshServingLow : 7
                    cellReselectionPriority : 6
                  intraFreqCellReselectionInfo
                    q-RxLevMin : -64
                    allowedMeasBandwidth : mbw50
                    presenceAntennaPort1 : false
                    neighCellConfig : 80(2 bits)
                    t-ReselectionEUTRA : 2
                  s-IntraSearch-v920
                    s-IntraSearchP-r9 : 31
                    s-IntraSearchQ-r9 : 0
                  s-NonIntraSearch-v920
                    s-NonIntraSearchP-r9 : 8
                    s-NonIntraSearchQ-r9 : 0

SYSTEM INFORMATION
LTE RRC Signaling Messages
  Version : 15
  RRC Release Number : 13
  RRC Version Minor : 1
  RRC Version Major : 2
  RB ID : 0
  Physical Cell ID : 365
  E-ARFCN : 103
  SFN : 0
  Channel : 2
  Bitmask of SIBS : 32
  Message Length : 28
  bcch-dl-sch
    message
      c1
        systemInformation
          criticalExtensions
            systemInformation-r8
              sib-TypeAndInfo[0]
                sib5
                  interFreqCarrierFreqList
                    InterFreqCarrierFreqList[0]
                      dl-CarrierFreq : 37950
                      q-RxLevMin : -64
                      t-ReselectionEUTRA : 2
                      threshX-High : 7
                      threshX-Low : 0
                      allowedMeasBandwidth : mbw100
                      presenceAntennaPort1 : false
                      cellReselectionPriority : 7
                      neighCellConfig : 80(2 bits)
                    InterFreqCarrierFreqList[1]
                      dl-CarrierFreq : 128
                      q-RxLevMin : -64
                      t-ReselectionEUTRA : 2
                      threshX-High : 2
                      threshX-Low : 0
                      allowedMeasBandwidth : mbw25
                      presenceAntennaPort1 : false
                      cellReselectionPriority : 6
                      neighCellConfig : 80(2 bits)
                  lateNonCriticalExtension
                    interFreqCarrierFreqList-v8h0[0]
                      multiBandInfoList
                        MultiBandInfoList[0]
                          FreqBandIndicator : 41
                    interFreqCarrierFreqList-v8h0[1]
                      multiBandInfoList
                        MultiBandInfoList[0]
                          FreqBandIndicator : 64
                    nonCriticalExtension
                      interFreqCarrierFreqList-v9e0[0]
                      interFreqCarrierFreqList-v9e0[1]
                        multiBandInfoList-v9e0
                          MultiBandInfoList-v9e0[0]
                            freqBandIndicator-v9e0 : 65

SYSTEM INFORMATION
LTE RRC Signaling Messages
  Version : 15
  RRC Release Number : 13
  RRC Version Minor : 1
  RRC Version Major : 2
  RB ID : 0
  Physical Cell ID : 459
  E-ARFCN : 37950
  SFN : 0
  Channel : 2
  Bitmask of SIBS : 16
  Message Length : 7
  bcch-dl-sch
    message
      c1
        systemInformation
          criticalExtensions
            systemInformation-r8
              sib-TypeAndInfo[0]
                sib4
                  intraFreqNeighCellList
                    IntraFreqNeighCellList[0]
                      physCellId : 461
                      q-OffsetCell : dB3
                    IntraFreqNeighCellList[1]
                      physCellId : 460
                      q-OffsetCell : dB1

SYSTEM INFORMATION
LTE RRC Signaling Messages
  Version : 15
  RRC Release Number : 13
  RRC Version Minor : 1
  RRC Version Major : 2
  RB ID : 0
  Physical Cell ID : 365
  E-ARFCN : 103
  SFN : 0
  Channel : 2
  Bitmask of SIBS : 64
  Message Length : 15
  bcch-dl-sch
    message
      c1
        systemInformation
          criticalExtensions
            systemInformation-r8
              sib-TypeAndInfo[0]
                sib6
                  carrierFreqListUTRA-FDD
                    CarrierFreqListUTRA-FDD[0]
                      carrierFreq : 10564
                      cellReselectionPriority : 4
                      threshX-High : 2
                      threshX-Low : 1
                      q-RxLevMin : -58
                      p-MaxUTRA : 33
                      q-QualMin : -18
                    CarrierFreqListUTRA-FDD[1]
                      carrierFreq : 2988
                      cellReselectionPriority : 4
                      threshX-High : 2
                      threshX-Low : 1
                      q-RxLevMin : -58
                      p-MaxUTRA : 33
                      q-QualMin : -18
                  t-ReselectionUTRA : 2

———————————————————————————
UMTS 900
———————————————————————————

SYSTEM INFORMATION 19
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 18
  sysInfoType19
    utra-PriorityInfoList
      utra-ServingCell
        priority : 4
        s-PrioritySearch1 : 7
        threshServingLow : 8
    eutra-FrequencyAndPriorityInfoList
      EUTRA-FrequencyAndPriorityInfoList[0]
        earfcn : 37950
        priority : 7
        qRxLevMinEUTRA : -64
        threshXhigh : 7
        threshXlow : 3
        eutraDetection : true
      EUTRA-FrequencyAndPriorityInfoList[1]
        earfcn : 128
        priority : 6
        qRxLevMinEUTRA : -64
        threshXhigh : 10
        threshXlow : 3
        eutraDetection : true
      EUTRA-FrequencyAndPriorityInfoList[2]
        earfcn : 103
        priority : 6
        qRxLevMinEUTRA : -64
        threshXhigh : 9
        threshXlow : 3
        eutraDetection : true

———————————————————————————
UMTS 2100
———————————————————————————

SYSTEM INFORMATION 11
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 81
  sysInfoType11
    sib12indicator : true
    fach-MeasurementOccasionInfo
      inter-freq-FDD-meas-ind : false
      inter-freq-TDD-meas-ind : false
      inter-RAT-meas-ind[0]
        RAT-Type : gsm
    measurementControlSysInfo
      use-of-HCS
        hcs-not-used
          cellSelectQualityMeasure
            cpich-Ec-N0
              intraFreqMeasurementSysInfo
                intraFreqCellInfoSI-List
                  removedIntraFreqCellList
                  newIntraFreqCellList
                    NewIntraFreqCellSI-List-ECN0[0]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 211
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[1]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 323
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[2]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 380
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[3]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 143
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[4]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 105
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[5]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 204
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[6]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 427
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[7]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 511
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[8]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 163
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[9]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 318
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[10]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 334
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[11]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 196
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[12]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 247
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[13]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 96
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[14]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 359
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[15]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 219
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[16]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 346
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[17]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 388
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[18]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 309
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[19]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 88
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[20]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 132
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[21]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 147
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false

                intraFreqMeasQuantity
                  filterCoefficient : fc2
                  modeSpecificInfo
                    fdd
                      intraFreqMeasQuantity-FDD : cpich-Ec-N0
                intraFreqReportingQuantityForRACH
                  sfn-SFN-OTD-Type : noReport
                  modeSpecificInfo
                    fdd
                      intraFreqRepQuantityRACH-FDD : cpich-EcN0
                maxReportedCellsOnRACH : currentCell
                reportingInfoForCellDCH
                  intraFreqReportingQuantity
                    activeSetReportingQuantities
                      dummy : noReport
                      cellIdentity-reportingIndicator : false
                      cellSynchronisationInfoReportingIndicator : true
                      modeSpecificInfo
                        fdd
                          cpich-Ec-N0-reportingIndicator : true
                          cpich-RSCP-reportingIndicator : true
                          pathloss-reportingIndicator : false
                    monitoredSetReportingQuantities
                      dummy : noReport
                      cellIdentity-reportingIndicator : false
                      cellSynchronisationInfoReportingIndicator : true
                      modeSpecificInfo
                        fdd
                          cpich-Ec-N0-reportingIndicator : true
                          cpich-RSCP-reportingIndicator : true
                          pathloss-reportingIndicator : false
                    detectedSetReportingQuantities
                      dummy : noReport
                      cellIdentity-reportingIndicator : false
                      cellSynchronisationInfoReportingIndicator : true
                      modeSpecificInfo
                        fdd
                          cpich-Ec-N0-reportingIndicator : true
                          cpich-RSCP-reportingIndicator : true
                          pathloss-reportingIndicator : false
                  measurementReportingMode
                    measurementReportTransferMode : acknowledgedModeRLC
                    periodicalOrEventTrigger : eventTrigger
                  reportCriteria
                    intraFreqReportingCriteria
                      eventCriteriaList
                        IntraFreqEventCriteriaList[0]
                          event
                            e1a
                              triggeringCondition : detectedSetAndMonitoredSetCells
                              reportingRange : 6
                              w : 0
                              reportDeactivationThreshold : t4
                              reportingAmount : ra-Infinity
                              reportingInterval : ri1
                          hysteresis : 0
                          timeToTrigger : tt320
                          reportingCellStatus
                            allActivePlusMonitoredAndOrDetectedSet : viactCellsPlus3
                        IntraFreqEventCriteriaList[1]
                          event
                            e1b
                              triggeringCondition : activeSetCellsOnly
                              reportingRange : 10
                              w : 0
                          hysteresis : 0
                          timeToTrigger : ttt640
                          reportingCellStatus
                            withinActiveSet : e3
                        IntraFreqEventCriteriaList[2]
                          event
                          hysteresis : 15
                          timeToTrigger : ttt2560
                          reportingCellStatus
                            allActivePlusMonitoredAndOrDetectedSet : viactCellsPlus1
              interFreqMeasurementSysInfo
                interFreqCellInfoSI-List
                  removedInterFreqCellList
                  newInterFreqCellList
                    NewInterFreqCellSI-List-ECN0[0]
                      frequencyInfo
                        modeSpecificInfo
                          fdd
                            uarfcn-UL : 2763
                            uarfcn-DL : 2988
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 211
                            primaryCPICH-TX-Power : 33
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false

SYSTEM INFORMATION 19
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 18
  sysInfoType19
    utra-PriorityInfoList
      utra-ServingCell
        priority : 4
        s-PrioritySearch1 : 7
        threshServingLow : 8
    eutra-FrequencyAndPriorityInfoList
      EUTRA-FrequencyAndPriorityInfoList[0]
        earfcn : 37950
        priority : 7
        qRxLevMinEUTRA : -64
        threshXhigh : 7
        threshXlow : 3
        eutraDetection : true
      EUTRA-FrequencyAndPriorityInfoList[1]
        earfcn : 128
        priority : 6
        qRxLevMinEUTRA : -64
        threshXhigh : 10
        threshXlow : 3
        eutraDetection : true
      EUTRA-FrequencyAndPriorityInfoList[2]
        earfcn : 103
        priority : 6
        qRxLevMinEUTRA : -64
        threshXhigh : 9
        threshXlow : 3
        eutraDetection : true