MASTER INFORMATION BLOCK
LTE MIB Message
  Version : 2
  Physical Cell ID : 121
  E-ARFCN : 6350
  SFN : 532
  Num TX Antennas : 2
  DL Bandwidth : 10 MHz (50)

SYSTEM INFORMATION BLOCK TYPE 1
LTE RRC Signaling Messages
  Version : 15
  RRC Release Number : 13
  RRC Version Minor : 1
  RRC Version Major : 2
  RB ID : 0
  Physical Cell ID : 121
  E-ARFCN : 6350
  SFN : 24965
  Channel : 2
  Bitmask of SIBS : 2
  Message Length : 22
  bcch-dl-sch
    message
      c1
        systemInformationBlockType1
          cellAccessRelatedInfo
            plmn-IdentityList
              PLMN-IdentityList[0]
                plmn-Identity
                  mcc
                    MCC[0]
                      MCC-MNC-Digit : 2
                    MCC[1]
                      MCC-MNC-Digit : 2
                    MCC[2]
                      MCC-MNC-Digit : 6
                  mnc
                    MNC[0]
                      MCC-MNC-Digit : 1
                    MNC[1]
                      MCC-MNC-Digit : 0
                cellReservedForOperatorUse : notReserved
            trackingAreaCode : '396D'H (14701)
            cellIdentity : '0CDC30A'H (13484810)
            cellBarred : notBarred
            intraFreqReselection : allowed
            csg-Indication : false
          cellSelectionInfo
            q-RxLevMin : -64
          freqBandIndicator : 20
          schedulingInfoList
            SchedulingInfoList[0]
              si-Periodicity : rf16
              sib-MappingInfo
                SIB-MappingInfo[0]
                  SIB-Type : sibType3
            SchedulingInfoList[1]
              si-Periodicity : rf32
              sib-MappingInfo
                SIB-MappingInfo[0]
                  SIB-Type : sibType5
            SchedulingInfoList[2]
              si-Periodicity : rf64
              sib-MappingInfo
                SIB-MappingInfo[0]
                  SIB-Type : sibType6
                SIB-MappingInfo[1]
                  SIB-Type : sibType7
          si-WindowLength : ms40
          systemInfoValueTag : 28

SYSTEM INFORMATION
LTE RRC Signaling Messages
  Version : 15
  RRC Release Number : 13
  RRC Version Minor : 1
  RRC Version Major : 2
  RB ID : 0
  Physical Cell ID : 121
  E-ARFCN : 6350
  SFN : 25154
  Channel : 2
  Bitmask of SIBS : 32
  Message Length : 22
  bcch-dl-sch
    message
      c1
        systemInformation
          criticalExtensions
            systemInformation-r8
              sib-TypeAndInfo[0]
                sib5
                  interFreqCarrierFreqList
                    InterFreqCarrierFreqList[0]
                      dl-CarrierFreq : 1600
                      q-RxLevMin : -64
                      t-ReselectionEUTRA : 1
                      threshX-High : 9
                      threshX-Low : 7
                      allowedMeasBandwidth : mbw100
                      presenceAntennaPort1 : false
                      cellReselectionPriority : 6
                      neighCellConfig : '01'B (1)
                      q-QualMin-r9 : -18
                    InterFreqCarrierFreqList[1]
                      dl-CarrierFreq : 2950
                      q-RxLevMin : -64
                      t-ReselectionEUTRA : 1
                      threshX-High : 9
                      threshX-Low : 7
                      allowedMeasBandwidth : mbw100
                      presenceAntennaPort1 : false
                      cellReselectionPriority : 6
                      neighCellConfig : '01'B (1)
                      q-QualMin-r9 : -18

SYSTEM INFORMATION
LTE RRC Signaling Messages
  Version : 15
  RRC Release Number : 13
  RRC Version Minor : 1
  RRC Version Major : 2
  RB ID : 0
  Physical Cell ID : 121
  E-ARFCN : 6350
  SFN : 25730
  Channel : 2
  Bitmask of SIBS : 192
  Message Length : 37
  bcch-dl-sch
    message
      c1
        systemInformation
          criticalExtensions
            systemInformation-r8
              sib-TypeAndInfo[0]
                sib6
                  carrierFreqListUTRA-FDD
                    CarrierFreqListUTRA-FDD[0]
                      carrierFreq : 10713
                      cellReselectionPriority : 4
                      threshX-High : 2
                      threshX-Low : 2
                      q-RxLevMin : -60
                      p-MaxUTRA : 24
                      q-QualMin : -16
                  t-ReselectionUTRA : 2
              sib-TypeAndInfo[1]
                sib7
                  t-ReselectionGERAN : 7
                  carrierFreqsInfoList
                    CarrierFreqsInfoListGERAN[0]
                      carrierFreqs
                        startingARFCN : 75
                        bandIndicator : dcs1800
                        followingARFCNs
                          explicitListOfARFCNs
                            ExplicitListOfARFCNs[0]
                              ARFCN-ValueGERAN : 76
                            ExplicitListOfARFCNs[1]
                              ARFCN-ValueGERAN : 77
                            ExplicitListOfARFCNs[2]
                              ARFCN-ValueGERAN : 78
                            ExplicitListOfARFCNs[3]
                              ARFCN-ValueGERAN : 79
                            ExplicitListOfARFCNs[4]
                              ARFCN-ValueGERAN : 80
                            ExplicitListOfARFCNs[5]
                              ARFCN-ValueGERAN : 81
                            ExplicitListOfARFCNs[6]
                              ARFCN-ValueGERAN : 82
                            ExplicitListOfARFCNs[7]
                              ARFCN-ValueGERAN : 83
                            ExplicitListOfARFCNs[8]
                              ARFCN-ValueGERAN : 84
                            ExplicitListOfARFCNs[9]
                              ARFCN-ValueGERAN : 85
                            ExplicitListOfARFCNs[10]
                              ARFCN-ValueGERAN : 86
                            ExplicitListOfARFCNs[11]
                              ARFCN-ValueGERAN : 87
                            ExplicitListOfARFCNs[12]
                              ARFCN-ValueGERAN : 88
                            ExplicitListOfARFCNs[13]
                              ARFCN-ValueGERAN : 89
                      commonInfo
                        ncc-Permitted : 'FF'H (255)
                        q-RxLevMin : 0
                        threshX-High : 7
                        threshX-Low : 7