MASTER INFORMATION BLOCK
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 24
  mib
    mib-ValueTag : 2
    plmn-Type
      gsm-MAP
        plmn-Identity
          mcc
            MCC[0]
              Digit : 2
            MCC[1]
              Digit : 2
            MCC[2]
              Digit : 6
          mnc
            MNC[0]
              Digit : 0
            MNC[1]
              Digit : 6
    sibSb-ReferenceList
      SIBSb-ReferenceList[0]
        sibSb-Type
          sysInfoTypeSB1 : 4
        scheduling
          scheduling
            sib-Pos
              rep128 : 63
      SIBSb-ReferenceList[1]
        sibSb-Type
          sysInfoType1 : 2
        scheduling
          scheduling
            sib-Pos
              rep32 : 2
      SIBSb-ReferenceList[2]
        sibSb-Type
          sysInfoType3 : 2
        scheduling
          scheduling
            sib-Pos
              rep16 : 1
      SIBSb-ReferenceList[3]
        sibSb-Type
          sysInfoType5 : 4
        scheduling
          scheduling
            segCount : 3
            sib-Pos
              rep32 : 3
      SIBSb-ReferenceList[4]
        sibSb-Type
        scheduling
          scheduling
            sib-Pos
              rep16 : 1
      SIBSb-ReferenceList[5]
        sibSb-Type
          sysInfoType11 : 4
        scheduling
          scheduling
            segCount : 8
            sib-Pos
              rep128 : 10
            sib-PosOffsetInfo
              SibOFF-List[0]
                SibOFF : so2
              SibOFF-List[1]
                SibOFF : so4
              SibOFF-List[2]
                SibOFF : so2
              SibOFF-List[3]
                SibOFF : so2
              SibOFF-List[4]
                SibOFF : so22
              SibOFF-List[5]
                SibOFF : so2
              SibOFF-List[6]
                SibOFF : so4

SYS.INFO.TYPE SB1
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 13
  sysInfoSB1
    sib-ReferenceList
      SIB-ReferenceList[0]
        sib-Type
          sysInfoType2 : 4
        scheduling
          scheduling
            sib-Pos
              rep128 : 59
      SIB-ReferenceList[1]
        sib-Type
          sysInfoType12 : 4
        scheduling
          scheduling
            sib-Pos
              rep32 : 7
      SIB-ReferenceList[2]
        sib-Type
          sysInfoType18 : 3
        scheduling
          scheduling
            sib-Pos
              rep128 : 59
    v6b0NonCriticalExtensions
      sysInfoTypeSB1-v6b0ext
      v860NonCriticalExtensions
        sysInfoTypeSB1-v860ext
          extSIBTypeInfoSchedulingInfo-List
            ExtSIBTypeInfoSchedulingInfo-List2[0]
              extensionSIB-Type2
              schedulingInfo
                scheduling
                  sib-Pos
                    rep128 : 61
              valueTagInfo
                cellValueTag : 1

SYS.INFO.TYPE 1
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 19
  sysInfoType1
    cn-CommonGSM-MAP-NAS-SysInfo : '1F4B'H (8011)
    cn-DomainSysInfoList
      CN-DomainSysInfoList[0]
        cn-DomainIdentity : cs-domain
        cn-Type
          gsm-MAP : '2801'H (10241)
        cn-DRX-CycleLengthCoeff : 6
      CN-DomainSysInfoList[1]
        cn-DomainIdentity : ps-domain
        cn-Type
          gsm-MAP : '0301'H (769)
        cn-DRX-CycleLengthCoeff : 6
    ue-ConnTimersAndConstants
      t-302 : ms1000
      n-302 : 7
      t-308 : ms40
      t-309 : 6
      t-313 : 2
      n-313 : s100
      t-314 : s6
      t-315 : s0
    ue-IdleTimersAndConstants
      t-300 : ms2000
      n-300 : 5
      t-312 : 10
      n-312 : s1
    v3a0NonCriticalExtensions
      sysInfoType1-v3a0ext
        ue-ConnTimersAndConstants-v3a0ext
        ue-IdleTimersAndConstants-v3a0ext
      v860NonCriticalExtentions
        sysInfoType1-v860ext
          ue-ConnTimersAndConstants
            t-323 : s5

SYS.INFO.TYPE 2
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 4
  sysInfoType2
    ura-IdentityList
      URA-IdentityList[0]
        URA-Identity : '1FA8'H (8104)

SYS.INFO.TYPE 3
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 16
  sysInfoType3
    sib4indicator : false
    cellIdentity : '0518773'H (5343091)
    cellSelectReselectInfo
      cellSelectQualityMeasure
        cpich-Ec-N0
      modeSpecificInfo
        fdd
          s-Intersearch : 5
          rat-List
            RAT-FDD-InfoList[0]
              rat-Identifier : gsm
              s-SearchRAT : 2
              s-HCS-RAT : -53
              s-Limit-SearchRAT : 0
          q-QualMin : -18
          q-RxlevMin : -58
      q-Hyst-l-S : 2
      t-Reselection-S : 2
      maxAllowedUL-TX-Power : 24
    cellAccessRestriction
      cellBarred
      cellReservedForOperatorUse : notReserved
      cellReservationExtension : notReserved
    v4b0NonCriticalExtensions
      sysInfoType3-v4b0ext
      v590NonCriticalExtension
        sysInfoType3-v590ext
        v5c0NoncriticalExtension
          sysInfoType3-v5c0ext
          v670NonCriticalExtension
            sysInfoType3-v670ext
            v770NonCriticalExtension
              sysInfoType3-v770ext
                deferredMeasurementControlReadingSupport
                  modeSpecificInfo
                    fdd
                      intraFreqMeasQuantity-FDD : cpich-Ec-N0

SYS.INFO.TYPE 5
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 71
  sysInfoType5
    sib6indicator : false
    pich-PowerOffset : -7
    modeSpecificInfo
      fdd
        aich-PowerOffset : -6
    primaryCCPCH-Info
      fdd
        tx-DiversityIndicator : false
    prach-SystemInformationList
      PRACH-SystemInformationList[0]
        prach-RACH-Info
          modeSpecificInfo
            fdd
              availableSignatures : 'FFFF'H (65535)
              availableSF : sfpr64
              preambleScramblingCodeWordNumber : 0
              puncturingLimit : pl1
              availableSubChannelNumbers : 'FFF'H (4095)
        transportChannelIdentity : 3
        rach-TransportFormatSet
          commonTransChTFS
            tti
              tti20
                CommonDynamicTF-InfoList[0]
                  rlc-Size
                    fdd
                      octetModeRLC-SizeInfoType2
                        sizeType1 : 15
                  numberOfTbSizeList[0]
                  logicalChannelList
                CommonDynamicTF-InfoList[1]
                  rlc-Size
                    fdd
                      octetModeRLC-SizeInfoType2
                        sizeType2 : 3
                  numberOfTbSizeList[0]
                  logicalChannelList
            semistaticTF-Information
              channelCodingType
                convolutional : half
              rateMatchingAttribute : 1
              crc-Size : crc16
        rach-TFCS
          normalTFCI-Signalling
            complete
              ctfcSize
                ctfc2Bit[0]
                  ctfc2 : 0
                  powerOffsetInformation
                    gainFactorInformation
                      signalledGainFactors
                        modeSpecificInfo
                          fdd
                            gainFactorBetaC : 11
                        gainFactorBetaD : 15
                    powerOffsetPp-m : 0
                ctfc2Bit[1]
                  ctfc2 : 1
                  powerOffsetInformation
                    gainFactorInformation
                      signalledGainFactors
                        modeSpecificInfo
                          fdd
                            gainFactorBetaC : 10
                        gainFactorBetaD : 15
                    powerOffsetPp-m : 0
        prach-Partitioning
          fdd[0]
        ac-To-ASC-MappingTable
          AC-To-ASC-MappingTable[0]
            AC-To-ASC-Mapping : 0
          AC-To-ASC-MappingTable[1]
            AC-To-ASC-Mapping : 0
          AC-To-ASC-MappingTable[2]
            AC-To-ASC-Mapping : 0
          AC-To-ASC-MappingTable[3]
            AC-To-ASC-Mapping : 0
          AC-To-ASC-MappingTable[4]
            AC-To-ASC-Mapping : 0
          AC-To-ASC-MappingTable[5]
            AC-To-ASC-Mapping : 0
          AC-To-ASC-MappingTable[6]
            AC-To-ASC-Mapping : 0
        modeSpecificInfo
          fdd
            primaryCPICH-TX-Power : 35
            constantValue : -27
            prach-PowerOffset
              powerRampStep : 2
              preambleRetransMax : 16
            rach-TransmissionParameters
              mmax : 16
              nb01Min : 0
              nb01Max : 0
            aich-Info
              channelisationCode256 : 2
              sttd-Indicator : false
              aich-TransmissionTiming : e1
    sCCPCH-SystemInformationList
      SCCPCH-SystemInformationList[0]
        secondaryCCPCH-Info
          modeSpecificInfo
            fdd
              dummy1 : mayBeUsed
              sttd-Indicator : false
              sf-AndCodeNumber
                sf128 : 4
              pilotSymbolExistence : false
              tfci-Existence : false
              positionFixedOrFlexible : fixed
              timingOffset : 20
        tfcs
          normalTFCI-Signalling
            complete
              ctfcSize
                ctfc2Bit[0]
                  ctfc2 : 0
                ctfc2Bit[1]
                  ctfc2 : 1
        fach-PCH-InformationList
          FACH-PCH-InformationList[0]
            transportFormatSet
              commonTransChTFS
                tti
                  tti10
                    CommonDynamicTF-InfoList[0]
                      rlc-Size
                        fdd
                          octetModeRLC-SizeInfoType2
                            sizeType1 : 24
                      numberOfTbSizeList[0]
                      numberOfTbSizeList[1]
                      logicalChannelList
                semistaticTF-Information
                  channelCodingType
                    convolutional : half
                  rateMatchingAttribute : 230
                  crc-Size : crc16
            transportChannelIdentity : 4
            ctch-Indicator : false
        pich-Info
          fdd
            channelisationCode256 : 3
            pi-CountPerFrame : e18
            sttd-Indicator : false
      SCCPCH-SystemInformationList[1]
        secondaryCCPCH-Info
          modeSpecificInfo
            fdd
              dummy1 : mayBeUsed
              sttd-Indicator : false
              sf-AndCodeNumber
                sf64 : 1
              pilotSymbolExistence : false
              tfci-Existence : true
              positionFixedOrFlexible : flexible
        tfcs
          normalTFCI-Signalling
            complete
              ctfcSize
                ctfc2Bit[0]
                  ctfc2 : 0
                ctfc2Bit[1]
                  ctfc2 : 1
                ctfc2Bit[2]
                  ctfc2 : 2
                ctfc2Bit[3]
                  ctfc2 : 3
        fach-PCH-InformationList
          FACH-PCH-InformationList[0]
            transportFormatSet
              commonTransChTFS
                tti
                  tti10
                    CommonDynamicTF-InfoList[0]
                      rlc-Size
                        fdd
                          octetModeRLC-SizeInfoType2
                            sizeType1 : 15
                      numberOfTbSizeList[0]
                      numberOfTbSizeList[1]
                      numberOfTbSizeList[2]
                        small : 2
                      logicalChannelList
                semistaticTF-Information
                  channelCodingType
                    convolutional : half
                  rateMatchingAttribute : 220
                  crc-Size : crc16
            transportChannelIdentity : 1
            ctch-Indicator : false
          FACH-PCH-InformationList[1]
            transportFormatSet
              commonTransChTFS
                tti
                  tti10
                    CommonDynamicTF-InfoList[0]
                      rlc-Size
                        fdd
                          octetModeRLC-SizeInfoType2
                            sizeType2 : 3
                      numberOfTbSizeList[0]
                      numberOfTbSizeList[1]
                      logicalChannelList
                semistaticTF-Information
                  channelCodingType
                  rateMatchingAttribute : 130
                  crc-Size : crc16
            transportChannelIdentity : 2
            ctch-Indicator : false
    v4b0NonCriticalExtensions
      sysInfoType5-v4b0ext
        frequencyBandIndicator : fdd2100
      v590NonCriticalExtensions
        v650NonCriticalExtensions
          v680NonCriticalExtensions
            sysInfoType5-v680ext
              hsdpa-CellIndicator : hsdpa-CapableCell
            v690NonCriticalExtensions
              sysInfoType5-v690ext
                edch-CellIndicator : edch-CapableCell

SYS.INFO.TYPE 7
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 4
  sysInfoType7
    modeSpecificInfo
      fdd
        ul-Interference : -107
    prach-Information-SIB5-List
      DynamicPersistenceLevelList[0]
        DynamicPersistenceLevel : 1

SYS.INFO.TYPE 11
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 211
  sysInfoType11
    sib12indicator : true
    fach-MeasurementOccasionInfo
      inter-freq-FDD-meas-ind : false
      inter-freq-TDD-meas-ind : false
      inter-RAT-meas-ind[0]
        RAT-Type : gsm
    measurementControlSysInfo
      use-of-HCS
        hcs-not-used
          cellSelectQualityMeasure
            cpich-Ec-N0
              intraFreqMeasurementSysInfo
                intraFreqCellInfoSI-List
                  removedIntraFreqCellList
                  newIntraFreqCellList
                    NewIntraFreqCellSI-List-ECN0[0]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 406
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[1]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 338
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[2]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 339
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[3]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 431
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[4]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 28
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[5]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 409
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[6]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 407
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[7]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 408
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[8]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 154
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[9]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 127
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[10]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 129
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[11]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 368
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[12]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 367
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[13]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 128
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[14]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 370
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[15]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 372
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[16]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 495
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[17]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 337
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false

                intraFreqMeasQuantity
                  filterCoefficient : fc2
                  modeSpecificInfo
                    fdd
                      intraFreqMeasQuantity-FDD : cpich-Ec-N0
                intraFreqReportingQuantityForRACH
                  sfn-SFN-OTD-Type : noReport
                  modeSpecificInfo
                    fdd
                      intraFreqRepQuantityRACH-FDD : cpich-EcN0
                maxReportedCellsOnRACH : currentCell
                reportingInfoForCellDCH
                  intraFreqReportingQuantity
                    activeSetReportingQuantities
                      dummy : noReport
                      cellIdentity-reportingIndicator : false
                      cellSynchronisationInfoReportingIndicator : true
                      modeSpecificInfo
                        fdd
                          cpich-Ec-N0-reportingIndicator : true
                          cpich-RSCP-reportingIndicator : true
                          pathloss-reportingIndicator : false
                    monitoredSetReportingQuantities
                      dummy : noReport
                      cellIdentity-reportingIndicator : false
                      cellSynchronisationInfoReportingIndicator : true
                      modeSpecificInfo
                        fdd
                          cpich-Ec-N0-reportingIndicator : true
                          cpich-RSCP-reportingIndicator : true
                          pathloss-reportingIndicator : false
                    detectedSetReportingQuantities
                      dummy : noReport
                      cellIdentity-reportingIndicator : false
                      cellSynchronisationInfoReportingIndicator : true
                      modeSpecificInfo
                        fdd
                          cpich-Ec-N0-reportingIndicator : true
                          cpich-RSCP-reportingIndicator : true
                          pathloss-reportingIndicator : false
                  measurementReportingMode
                    measurementReportTransferMode : acknowledgedModeRLC
                    periodicalOrEventTrigger : eventTrigger
                  reportCriteria
                    intraFreqReportingCriteria
                      eventCriteriaList
                        IntraFreqEventCriteriaList[0]
                          event
                            e1a
                              triggeringCondition : detectedSetAndMonitoredSetCells
                              reportingRange : 6
                              w : 0
                              reportDeactivationThreshold : t4
                              reportingAmount : ra-Infinity
                              reportingInterval : ri1
                          hysteresis : 0
                          timeToTrigger : tt320
                          reportingCellStatus
                            allActivePlusMonitoredAndOrDetectedSet : viactCellsPlus3
                        IntraFreqEventCriteriaList[1]
                          event
                            e1b
                              triggeringCondition : activeSetCellsOnly
                              reportingRange : 10
                              w : 0
                          hysteresis : 0
                          timeToTrigger : ttt640
                          reportingCellStatus
                            withinActiveSet : e3
                        IntraFreqEventCriteriaList[2]
                          event
                          hysteresis : 15
                          timeToTrigger : ttt2560
                          reportingCellStatus
                            allActivePlusMonitoredAndOrDetectedSet : viactCellsPlus1

              interFreqMeasurementSysInfo
                interFreqCellInfoSI-List
                  removedInterFreqCellList
                  newInterFreqCellList
                    NewInterFreqCellSI-List-ECN0[0]
                      frequencyInfo
                        modeSpecificInfo
                          fdd
                            uarfcn-DL : 10664
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 406
                            primaryCPICH-TX-Power : 35
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[1]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 407
                            primaryCPICH-TX-Power : 35
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[2]
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 408
                            primaryCPICH-TX-Power : 35
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false

          interRATMeasurementSysInfo
            interRATCellInfoList
              removedInterRATCellList
              newInterRATCellList
                NewInterRATCellList-B[0]
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 7
                        maxAllowedUL-TX-Power : 33
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -54
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 7
                        bcc : 1
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 44
                NewInterRATCellList-B[1]
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 7
                        maxAllowedUL-TX-Power : 33
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -54
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 7
                        bcc : 1
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 73
                NewInterRATCellList-B[2]
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 7
                        maxAllowedUL-TX-Power : 33
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -54
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 6
                        bcc : 1
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 29
                NewInterRATCellList-B[3]
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 7
                        maxAllowedUL-TX-Power : 33
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -54
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 6
                        bcc : 1
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 52
                NewInterRATCellList-B[4]
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 7
                        modeSpecificInfo
                          gsm
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 6
                        bcc : 7
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 48
                NewInterRATCellList-B[5]
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 7
                        modeSpecificInfo
                          gsm
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 6
                        bcc : 7
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 50
                NewInterRATCellList-B[6]
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 7
                        maxAllowedUL-TX-Power : 33
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -54
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 3
                        bcc : 1
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 45
                NewInterRATCellList-B[7]
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 7
                        maxAllowedUL-TX-Power : 33
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -54
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 4
                        bcc : 7
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 54
                NewInterRATCellList-B[8]
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 7
                        maxAllowedUL-TX-Power : 33
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -54
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 7
                        bcc : 6
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 54
                NewInterRATCellList-B[9]
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 7
                        maxAllowedUL-TX-Power : 33
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -54
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 4
                        bcc : 0
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 26
                NewInterRATCellList-B[10]
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 7
                        maxAllowedUL-TX-Power : 33
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -54
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 7
                        bcc : 2
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 30
                NewInterRATCellList-B[11]
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 7
                        maxAllowedUL-TX-Power : 33
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -54
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 7
                        bcc : 2
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 54
                NewInterRATCellList-B[12]
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 7
                        maxAllowedUL-TX-Power : 33
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -54
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 7
                        bcc : 2
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 71
                NewInterRATCellList-B[13]
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 7
                        modeSpecificInfo
                          gsm
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 7
                        bcc : 0
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 70
                NewInterRATCellList-B[14]
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 7
                        maxAllowedUL-TX-Power : 33
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -54
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 1
                        bcc : 2
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 56
                NewInterRATCellList-B[15]
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 7
                        modeSpecificInfo
                          gsm
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 7
                        bcc : 0
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 46
                NewInterRATCellList-B[16]
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 7
                        maxAllowedUL-TX-Power : 33
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -54
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 3
                        bcc : 2
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 30
                NewInterRATCellList-B[17]
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 7
                        maxAllowedUL-TX-Power : 33
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -54
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 4
                        bcc : 4
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 72
                NewInterRATCellList-B[18]
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 7
                        maxAllowedUL-TX-Power : 33
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -54
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 4
                        bcc : 4
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 53
                NewInterRATCellList-B[19]
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 7
                        maxAllowedUL-TX-Power : 33
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -54
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 3
                        bcc : 2
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 52

SYS.INFO.TYPE 12
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 9
  sysInfoType12
    fach-MeasurementOccasionInfo
      inter-freq-FDD-meas-ind : false
      inter-freq-TDD-meas-ind : false
      inter-RAT-meas-ind[0]
        RAT-Type : gsm
    measurementControlSysInfo
      use-of-HCS
        hcs-not-used
          cellSelectQualityMeasure
            cpich-Ec-N0
      trafficVolumeMeasSysInfo
        trafficVolumeMeasurementObjectList
          TrafficVolumeMeasurementObjectList[0]
        trafficVolumeMeasQuantity
        trafficVolumeReportingQuantity
          rlc-RB-BufferPayload : true
          rlc-RB-BufferPayloadAverage : false
          rlc-RB-BufferPayloadVariance : false
        measurementValidity
          ue-State : all-But-Cell-DCH
        measurementReportingMode
          measurementReportTransferMode : acknowledgedModeRLC
          periodicalOrEventTrigger : eventTrigger
        reportCriteriaSysInf
          trafficVolumeReportingCriteria
            transChCriteriaList
              TransChCriteriaList[0]
                ul-transportChannelID
                eventSpecificParameters[0]
                  eventID : e4a
                  reportingThreshold : th64
                  pendingTimeAfterTrigger : ptat1

SYS.INFO.TYPE 18
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 8
  sysInfoType18
    idleModePLMNIdentities
      plmnsOfInterRATCellsList
        PLMNsOfInterRATCellsList[0]
          plmn-Identity
            mcc
              MCC[0]
                Digit : 2
              MCC[1]
                Digit : 2
              MCC[2]
                Digit : 6
            mnc
              MNC[0]
                Digit : 0
              MNC[1]
                Digit : 3
        PLMNsOfInterRATCellsList[1]
        PLMNsOfInterRATCellsList[2]
        PLMNsOfInterRATCellsList[3]
        PLMNsOfInterRATCellsList[4]
        PLMNsOfInterRATCellsList[5]
        PLMNsOfInterRATCellsList[6]
        PLMNsOfInterRATCellsList[7]
        PLMNsOfInterRATCellsList[8]
        PLMNsOfInterRATCellsList[9]
        PLMNsOfInterRATCellsList[10]
        PLMNsOfInterRATCellsList[11]
        PLMNsOfInterRATCellsList[12]
        PLMNsOfInterRATCellsList[13]
        PLMNsOfInterRATCellsList[14]
        PLMNsOfInterRATCellsList[15]
        PLMNsOfInterRATCellsList[16]
        PLMNsOfInterRATCellsList[17]
        PLMNsOfInterRATCellsList[18]
        PLMNsOfInterRATCellsList[19]

SYS.INFO.TYPE 19
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 14
  sysInfoType19
    utra-PriorityInfoList
      utra-ServingCell
        priority : 3
        s-PrioritySearch1 : 8
        threshServingLow : 8
    eutra-FrequencyAndPriorityInfoList
      EUTRA-FrequencyAndPriorityInfoList[0]
        earfcn : 6425
        priority : 5
        qRxLevMinEUTRA : -63
        threshXhigh : 7
        threshXlow : 3
        eutraDetection : true
      EUTRA-FrequencyAndPriorityInfoList[1]
        earfcn : 1798
        priority : 6
        qRxLevMinEUTRA : -63
        threshXhigh : 6
        threshXlow : 3
        eutraDetection : true

————————————————————————————————
BlackBerry 9780
————————————————————————————————

CELL INFORMATION

3G CS+PS noPDP IDLE
RRC State: IDLE

PSC=406 UARFCN=(1)10664 RSSI=-59
MCC: 226  MNC:6f LAC: 1f4b RAC:0003
NCO: 0  NMO: 1
MSC Rev: 99+ SGSN Rev: 99+

URA_ID: later
DRX Cycle Length: 64

SIB VALIDITY

Uarfcn = 10664 and Psc = 406
MIB validity = Valid
SIB1 validity = Valid
SIB2 validity = Valid
SIB3 validity = Valid
SIB4 validity = Invalid
SIB5 validity = Valid
SIB6 validity = Invalid
SIB7 validity = Invalid
SIB11 validity = Valid
SIB12 validity = Valid
SIB13 validity = Invalid
SIB13.1 validity = Invalid
SIB13.2 validity = Invalid
SIB13.3 validity = Invalid
SIB13.4 validity = Invalid
SIB14 validity = Invalid
SIB15 validity = Invalid
SIB15.1 validity = Invalid
SIB15.2 validity = Invalid
SIB15.3 validity = Invalid
SIB16 validity = Invalid
SIB17 validity = Invalid
SIB15.4 validity = Invalid
SIB18 validity = Valid
SB1 validity = Valid
SB2 validity = Invalid
SIB15.5 validity = Invalid

MIB

MIB Value Tag: 2
MCC:2 2 6  MNC:0  d 6 
SIB1 scheduled with tag 2
SIB2 not scheduled in MIB
SIB3 scheduled with tag 2
SIB4 not scheduled in MIB
SIB5 scheduled with tag 4
SIB6 not scheduled in MIB
SIB7 scheduled with tag 0
SIB11 scheduled with tag 4
SIB12 not scheduled in MIB
SIB13 not scheduled in MIB
SIB13.1 not scheduled in MIB
SIB13.2 not scheduled in MIB
SIB13.3 not scheduled in MIB
SIB13.4 not scheduled in MIB
SIB14 not scheduled in MIB
SIB15 not scheduled in MIB
SIB16 not scheduled in MIB
SIB17 not scheduled in MIB
SB1 scheduled with tag 4
SB2 not scheduled in MIB
SIB15.1 not scheduled in MIB
SIB15.2 not scheduled in MIB
SIB15.2 not scheduled in MIB
SIB15.4 not scheduled in MIB
SIB18 not scheduled in MIB
SIB15.5 not scheduled in MIB

SCHEDULING BLK 1

SIB1 not scheduled in sb1
SIB2 scheduled with tag 4
SIB3 not scheduled in sb1
SIB4 not scheduled in sb1
SIB5 not scheduled in sb1
SIB6 not scheduled in sb1
SIB7 not scheduled in sb1
SIB11 not scheduled in sb1
SIB12 scheduled with tag 4
SIB13 not scheduled in sb1
SIB13.1 not scheduled in sb1
SIB13.2 not scheduled in sb1
SIB13.3 not scheduled in sb1
SIB13.4 not scheduled in sb1
SIB14 not scheduled in sb1
SIB15 not scheduled in sb1
SIB16 not scheduled in sb1
SIB17 not scheduled in sb1
SB1 not scheduled in sb1
sb1 not scheduled in sb1
SIB15.1 not scheduled in sb1
SIB15.2 not scheduled in sb1
SIB15.2 not scheduled in sb1
SIB15.4 not scheduled in sb1
SIB18 scheduled with tag 3
SIB15.5 not scheduled in sb1

SB 2 not present

SIB 1

T300: 2000
N300: 5
T302: 1000
N302: 7

SIB 3

Cell Identity: 5343091
Sib4Indicator: False
Barred Status: Not Barred
Reserve Indicator: Not reserved
Access Barred list: Absent
AccessBarredClassBitmap: 0
Cell Sel Critieria: CPICH-Ec/No
Qqualmin: -18
QrxlevMin: -58
Max UL TX Power: 24
s_IntraSearch: INVALID
s_InterSearch: 10
s_SearchHCS: INVALID
s_HCS_GSM: -105
s_Limit_SearchRAT: 0

SIB 4 not present

SIB 5

Sib6Indicator: False
Total Prach Config: 1
Step:2 RetranMax:16 mMax:16
PrachConfig2 Absent
PrachConfig3 Absent
PrachConfig4 Absent
PrachConfig5 Absent
PrachConfig6 Absent
PrachConfig7 Absent
PrachConfig8 Absent
PrachConfig9 Absent
PrachConfig10 Absent
PrachConfig11 Absent
PrachConfig12 Absent
PrachConfig13 Absent
PrachConfig14 Absent
PrachConfig15 Absent
PrachConfig16 Absent

Total Sccpch Config: 2
sttd_Indicator: FALSE
sttd_Indicator: FALSE
SccpchConfig 3 Absent
SccpchConfig 4 Absent
SccpchConfig 5 Absent
SccpchConfig 6 Absent
SccpchConfig 7 Absent
SccpchConfig 8 Absent
SccpchConfig 9 Absent
SccpchConfig 10 Absent
SccpchConfig 11 Absent
SccpchConfig 12 Absent
SccpchConfig 13 Absent
SccpchConfig 14 Absent
SccpchConfig 15 Absent
SccpchConfig 16 Absent

SIB 6 & 7 not present

SIB 11

Sib12Indicator: True
HCS Used: False
Quality Type: CPICH-ECNO
Intra-Frequency Cells: Present
Inter-Frequency Cells: Present
Inter-Rat Cells: Present

Total Intra-Freq Cell: 18
Cell1 PSC: 406
Cell2 PSC: 338
Cell3 PSC: 339
Cell4 PSC: 431
Cell5 PSC: 28
Cell6 PSC: 409
Cell7 PSC: 407
Cell8 PSC: 408
Cell9 PSC: 154
Cell10 PSC: 127
Cell11 PSC: 129
Cell12 PSC: 128
Cell13 PSC: 368
Cell14 PSC: 367
Cell15 PSC: 370
Cell16 PSC: 372
Cell17 PSC: 495
Cell18 PSC: 337

Total Inter-Freq Cell: 1
Cell1 UARFCN: 10639 PSC: 406

Total Inter-RAT Cell: 20
Cell1 Band:DCS1800 ARFCN:44 BSIC:7 1
Cell2 Band:DCS1800 ARFCN:73 BSIC:7 1
Cell3 Band:DCS1800 ARFCN:29 BSIC:6 1
Cell4 Band:DCS1800 ARFCN:52 BSIC:6 1
Cell5 Band:DCS1800 ARFCN:48 BSIC:6 7
Cell6 Band:DCS1800 ARFCN:50 BSIC:6 7
Cell7 Band:DCS1800 ARFCN:45 BSIC:3 1
Cell8 Band:DCS1800 ARFCN:54 BSIC:4 7
Cell9 Band:DCS1800 ARFCN:54 BSIC:7 6
Cell10 Band:DCS1800 ARFCN:26 BSIC:4 0
Cell11 Band:DCS1800 ARFCN:30 BSIC:7 2
Cell12 Band:DCS1800 ARFCN:54 BSIC:7 2
Cell13 Band:DCS1800 ARFCN:71 BSIC:7 2
Cell14 Band:DCS1800 ARFCN:70 BSIC:7 0
Cell15 Band:DCS1800 ARFCN:56 BSIC:1 2
Cell16 Band:DCS1800 ARFCN:46 BSIC:7 0
Cell17 Band:DCS1800 ARFCN:30 BSIC:3 2
Cell18 Band:DCS1800 ARFCN:72 BSIC:4 4
Cell19 Band:DCS1800 ARFCN:53 BSIC:4 4
Cell20 Band:DCS1800 ARFCN:52 BSIC:3 2

NEIGHBOUR CELLS

Active RAT is UTRAN - IDLE

IntraFreqCells 18 Uarfcn:10664 RSSI:-58
S PSC:406 EcNo:-7 RSCP:-65
  PSC:408 EcNo:-11 RSCP:-71
  PSC:338 EcNo:-40 RSCP:-167
  PSC:339 EcNo:-40 RSCP:-167
  PSC:431 EcNo:-40 RSCP:-167
  PSC:28 EcNo:-40 RSCP:-167
  PSC:409 EcNo:-40 RSCP:-167
  PSC:407 EcNo:-40 RSCP:-167
  PSC:154 EcNo:-40 RSCP:-167
  PSC:127 EcNo:-40 RSCP:-167
  PSC:129 EcNo:-40 RSCP:-167
  PSC:128 EcNo:-40 RSCP:-167
  PSC:368 EcNo:-40 RSCP:-167
  PSC:367 EcNo:-40 RSCP:-167
  PSC:370 EcNo:-40 RSCP:-167
  PSC:372 EcNo:-40 RSCP:-167
  PSC:495 EcNo:-40 RSCP:-167
  PSC:337 EcNo:-40 RSCP:-167

InterFreq Cells : 3
Uarfcn:10639 RSSI:-65
PSC:406 EcNo:-7 RSCP:-72
PSC:408 EcNo:-12 RSCP:-77
PSC:407 EcNo:-40 RSCP:-167

InterRAT Cells 20 RSSI: -89
G ARFCN:48 RSSI:-89 BSIC: Verified
G ARFCN:70 RSSI:-53 BSIC: Not Verified
G ARFCN:73 RSSI:-84 BSIC: Not Verified
G ARFCN:52 RSSI:-91 BSIC: Not Verified
G ARFCN:29 RSSI:-50 BSIC: Not Verified
G ARFCN:70 RSSI:-53 BSIC: Not Verified
G ARFCN:26 RSSI:-96 BSIC: Not Verified
G ARFCN:45 RSSI:-92 BSIC: Not Verified
G ARFCN:30 RSSI:-47 BSIC: Verified
G ARFCN:54 RSSI:-65 BSIC: Verified
G ARFCN:71 RSSI:-47 BSIC: Verified
G ARFCN:44 RSSI:-94 BSIC: Not Verified
G ARFCN:56 RSSI:-66 BSIC: Not Verified
G ARFCN:46 RSSI:-78 BSIC: Not Verified
G ARFCN:30 RSSI:-47 BSIC: Not Verified
G ARFCN:72 RSSI:-110 BSIC: Not Verified
G ARFCN:53 RSSI:-110 BSIC: Not Verified
G ARFCN:52 RSSI:-92 BSIC: Not Verified
G ARFCN:50 RSSI:-87 BSIC: Not Verified
G ARFCN:73 RSSI:-84 BSIC: Not Verified