SYSTEM INFORMATION TYPE 1
GSM RR Signaling Message
  Channel : 129
  Type : 25
  Length : 23
  Direction : 0
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 25
  System Information Type 1
    Cell Channel Description
      Gsm Format Id
        Spare : 0
        Bit Map 0
          Caarfcn 124 To 121 : 0
          Caarfcn 120 To 113 : 0
          Caarfcn 112 To 105 : 0
          Caarfcn 104 To 097 : 0
          Caarfcn 096 To 089 : 0
          Caarfcn 088 To 081 : 0
          Caarfcn 080 To 073 : 0
          Caarfcn 072 To 065 : 15
          Caarfcn 064 To 057 : 255
          Caarfcn 056 To 049 : 0
          Caarfcn 048 To 041 : 7
          Caarfcn 040 To 033 : 255
          Caarfcn 032 To 025 : 128
          Caarfcn 024 To 017 : 0
          Caarfcn 016 To 009 : 0
          Caarfcn 008 To 001 : 0
    Rach Control Parameter
      Max Retrans : Maximum 4 retransmissions (2)
      Tx Integer : 50 slots used to spread transmission (15)
      Cell Bar Access : The cell is not barred (0)
      Re : Call Reestablishment not allowed in the cell (1)
      Ac C : 0
    Si 1 Rest Octets
      Band Indicator : 1800 Band (0)

SYSTEM INFORMATION TYPE 2
GSM RR Signaling Message
  Channel : 129
  Type : 26
  Length : 23
  Direction : 0
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 26
  System Information Type 2
    Bcch Frequency List
      Bit 128 : 0
      Bit 127 : 0
      Ext Ind : The information element carries the complete BA (0)
      Ba Ind : 1
      Bit 124 To 121 : 0
      Bit 120 To 113 : 0
      Bit 112 To 105 : 0
      Bit 104 To 097 : 0
      Bit 096 To 089 : 0
      Bit 088 To 081 : 0
      Bit 080 To 073 : 1
      Bit 072 To 065 : 224
      Bit 064 To 057 : 0
      Bit 056 To 049 : 42
      Bit 048 To 041 : 208
      Bit 040 To 033 : 0
      Bit 032 To 025 : 10
      Bit 024 To 017 : 0
      Bit 016 To 009 : 0
      Bit 008 To 001 : 0
    Ncc Permitted
      Ncc Permited : 255
    Rach Control Parameter
      Max Retrans : Maximum 4 retransmissions (2)
      Tx Integer : 50 slots used to spread transmission (15)
      Cell Bar Access : The cell is not barred (0)
      Re : Call Reestablishment not allowed in the cell (1)
      Ac C : 0

SYSTEM INFORMATION TYPE 2 QuaTer
GSM RR Signaling Message
  Channel : 129
  Type : 7
  Length : 23
  Direction : 0
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 7
  System Information Type 2quater
    Si 2ter Quater Rest Octets
      Ba Ind : 1
      3g Ba Ind : 0
      Mp Change Mark : 0
      Si2quater Index : 2
      Si2quater Count : 3
      3G CCN Active : 0
      Priority and E-UTRAN Parameters Description
        Serving Cell Priority Parameters Description
          Geran Priority : 1
          Thresh Priority Search : 0
          Thresh GSM Low : 0
          H_PRIO : 0
          T_Reselection : 0
        3G Priority Parameters Description
          Utran Start : 1
          Utran Stop : 1
          Repeated UTRAN Priority Parameters[0]
            UTRAN Frequency Index : 0
            UTRAN Priority : 3
            Thresh UTRAN High : 4
            UTRAN Qrxlevmin : 0
          Repeated UTRAN Priority Parameters[1]
            Thresh UTRAN Low : 11
          Repeated UTRAN Priority Parameters[2]
            UTRAN Qrxlevmin : 7
          Repeated UTRAN Priority Parameters[3]
            UTRAN Frequency Index : 18
            UTRAN Frequency Index : 6
            UTRAN Frequency Index : 0
            UTRAN Frequency Index : 16
            UTRAN Frequency Index : 7
            UTRAN Frequency Index : 24

SYSTEM INFORMATION TYPE 2 QuaTer
GSM RR Signaling Message
  Channel : 131
  Type : 7
  Length : 23
  Direction : 0
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 7
  System Information Type 2quater
    Si 2ter Quater Rest Octets
      Ba Ind : 1
      3g Ba Ind : 0
      Mp Change Mark : 0
      Si2quater Index : 0
      Si2quater Count : 3
      3G Neighbour Cell Description
        UTRAN FDD Description
          FDD ARFCN : 10639
          FDD Indic0 : 0
          Nr Of Fdd Cells : 7
          W : 129
          W : 510
          W : 277
          W : 157
          W : 88
          W : 1
          W : 1
      3G Measurement Parameters Description
        Qsearch I : 7
        Qsearch C Initial : 1
        Fdd Qoffset Included : 1
        Fdd Qoffset : 0
        Fdd Rep Quant : 1
        Fdd Multirat Reporting : 1
        Fdd Qmin : 7
        Tdd Qoffset Included : 0
      GPRS 3G Measurement Parameters Description
        Qsearch P : 7
        Gsm 3g Search Prio : 1
        Fdd Rep Quant Included : 0
        Fdd Reporting Offset Included : 0
        Tdd Multirat Reporting Included : 0
        Tdd Reporting Offset Included : 0
      3G Additional Measurement Parameters Description
        FDD Qmin Offset : 0
        FDD RSCP min : 6
      3G Additional Measurement Parameters Description 2
        Fdd Reporting Threshold 2 : 26
      3G CCN Active : 0

SYSTEM INFORMATION TYPE 2 QuaTer
GSM RR Signaling Message
  Channel : 129
  Type : 7
  Length : 23
  Direction : 0
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 7
  System Information Type 2quater
    Si 2ter Quater Rest Octets
      Ba Ind : 1
      3g Ba Ind : 0
      Mp Change Mark : 0
      Si2quater Index : 1
      Si2quater Count : 3
      3G Neighbour Cell Description
        Index Start 3g : 7
        UTRAN FDD Description
          FDD ARFCN : 10639
          FDD Indic0 : 0
          Nr Of Fdd Cells : 2
          W : 409
          W : 511

SYSTEM INFORMATION TYPE 2 QuaTer
GSM RR Signaling Message
  Channel : 129
  Type : 7
  Length : 23
  Direction : 0
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 7
  System Information Type 2quater
    Si 2ter Quater Rest Octets
      Ba Ind : 1
      3g Ba Ind : 0
      Mp Change Mark : 0
      Si2quater Index : 3
      Si2quater Count : 3
      3G CCN Active : 0
      Priority and E-UTRAN Parameters Description
        E-UTRAN Parameters Description
          E-Utran CCN Active : 0
          E-Utran Start : 0
          E-Utran Stop : 1
          E-UTRAN Neighbour Cells[0]
            EARFCN : 1798
            Measurement Bandwidth : 0
            E-UTRAN_PRIORITY : 6
            THRESH_E-UTRAN_high : 6
            THRESH_E-UTRAN_low : 4
            E-UTRAN_QRXLEVMIN : 7
          E-UTRAN Neighbour Cells[1]
            EARFCN : 3650			——>   Band 8 (900MHz)
            Measurement Bandwidth : 0
            EARFCN : 6425
            Measurement Bandwidth : 0
            E-UTRAN_PRIORITY : 5
            THRESH_E-UTRAN_high : 7
            THRESH_E-UTRAN_low : 22
            E-UTRAN_QRXLEVMIN : 7

SYSTEM INFORMATION TYPE 3
GSM RR Signaling Message
  Channel : 129
  Type : 27
  Length : 23
  Direction : 0
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 27
  System Information Type 3
    Cell Identity : 34679
    Location Area Identification
      MCC : 226
      MNC : 3
      LAC : 18000
    Control Channel Description
      Mscr : MSC is Release '99 onwards (1)
      Att : MSs in the cell shall apply IMSI attach and detach procedure (1)
      Bs Ag Blks Res : 1
      Ccch Conf : 1 basic physical channel used for CCCH, not combined with SDCCHs (0)
      Spare : 0
      Cbq3 : Iu mode not supported (0)
      Spare : 0
      Bs Pa Mfrms : 3 multiframes period for transmission of PAGING REQUEST messages to the same paging subgroup (1)
      T3212 Timeout Value : UnKnOwN (40)
    Cell Options
      Dn-Ind : 0
      Pwrc : PWRC is not set (0)
      Dtx : The MSs shall use uplink discontinuous transmission (1)
      Radio Link Timeout : 4
    Cell Selection Parameters
      Cell Reselect Hysteresis : 8 dB RXLEV hysteresis for LA re-selection (4)
      Ms Txpwr Max Cch : 5
      Acs : System information type 16 and 17 are not broadcast on the BCCH (0)
      Neci : New establishment causes are supported (1)
      Rxlev Access Min : 0
    Rach Control Parameters
      Max Retrans : Maximum 4 retransmissions (2)
      Tx Integer : 50 slots used to spread transmission (15)
      Cell Bar Access : The cell is not barred (0)
      Re : Call Reestablishment not allowed in the cell (1)
      Ac C : 0
    Si 3 Rest Octets
      Selection Parameters Included : 1
      Cbq : 0
      Cell Reselect Offset : 0
      Temporary Offset : 0
      Penalty Time : 0
      Optional Power Offset Included : 0
      System Information 2ter Indicator : SYSTEM INFORMATION TYPE 2ter message is not available (0)
      Early Classmark Sending Control : Early Classmark Sending is forbidden (0)
      Where Included : 0
      Gprs Indicator Included : 0
      3g Early Classmark Sending Restriction : Neither UTRAN nor cdma2000 classmark change messages shall be sent with the Early classmark sending (0)
      Si2quater Indicator Included : 1
      Si2quater Position : SYSTEM INFORMATION TYPE 2 quater message is sent on BCCH Ext (1)

SYSTEM INFORMATION TYPE 4
GSM RR Signaling Message
  Channel : 129
  Type : 28
  Length : 23
  Direction : 0
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 28
  System Information Type 4
    Location Area Identification
      MCC : 226
      MNC : 3
      LAC : 18000
    Cell Selection Parameters
      Cell Reselect Hysteresis : 8 dB RXLEV hysteresis for LA re-selection (4)
      Ms Txpwr Max Cch : 5
      Acs : System information type 16 and 17 are not broadcast on the BCCH (0)
      Neci : New establishment causes are supported (1)
      Rxlev Access Min : 0
    Rach Control Parameters
      Max Retrans : Maximum 4 retransmissions (2)
      Tx Integer : 50 slots used to spread transmission (15)
      Cell Bar Access : The cell is not barred (0)
      Re : Call Reestablishment not allowed in the cell (1)
      Ac C : 0
    Cbch Channel Description
      Channel Type : 10
      Tn : 1
      Tsc : 2
      H : Single RF Channel (0)
      Spare : 0
      Afrcn : 71
    Si 4 Rest Octets
      Si4 Rest Octets O
        Cbq : 0
        Cell Reselect Offset : 0
        Temporary Offset : 0
        Penalty Time : 0
        Ra Colour : 3
        SI13 Position : 1

SYSTEM INFORMATION TYPE 5
GSM RR Signaling Message
  Channel : 132
  Type : 29
  Length : 18
  Direction : 0
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 29
  System Information Type 5
    Bcch Frequency List
      Bit 128 : 0
      Bit 127 : 0
      Ext Ind : The information element carries the complete BA (0)
      Ba Ind : 0
      Bit 124 To 121 : 0
      Bit 120 To 113 : 0
      Bit 112 To 105 : 0
      Bit 104 To 097 : 0
      Bit 096 To 089 : 0
      Bit 088 To 081 : 0
      Bit 080 To 073 : 1
      Bit 072 To 065 : 224
      Bit 064 To 057 : 0
      Bit 056 To 049 : 42
      Bit 048 To 041 : 208
      Bit 040 To 033 : 0
      Bit 032 To 025 : 10
      Bit 024 To 017 : 0
      Bit 016 To 009 : 0
      Bit 008 To 001 : 0

SYSTEM INFORMATION TYPE 6
GSM RR Signaling Message
  Channel : 132
  Type : 30
  Length : 18
  Direction : 0
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 30
  System Information Type 6
    Cell Identity : 34677
    Location Area Identification
      MCC : 226
      MNC : 3
      LAC : 18000
    Cell Options
      Dtx : 1
      Pwrc : PWRC is not set (0)
      Dtx : The MSs shall use uplink discontinuous transmission (1)
      Radio Link Timeout : 4
    Ncc Permitted
      Ncc Permited : 255
    Si 6 Rest Octets
      Pch And Nch Info Included : 0
      Vbs Vgcs Options Included : 0
      Dtm Support : DTM is supported in the serving cell (1)
      Rac : 89
      Max Lapdm : Any message segmented in up to 7 LAPDm frames (2)
      Band Indicator : 1900 Band (1)
      Implicit Spare : 149

SYSTEM INFORMATION TYPE 13
GSM RR Signaling Message
  Channel : 129
  Type : 0
  Length : 23
  Direction : 0
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 0
  System Information Type 13
    Si 13 Rest Octets
      BCCH Change Mark : 6
      Si Change Field : Update of unspecified SI message or SI messages (0)
      RAC : 1
      SPGC CCCH Sup : 0
      Priority Access Thr : 6
      Network Control Order : 0
      GPRS Cell Options
        Nmo : Network Mode of Operation II (1)
        T3168 : 0
        T3192 : 200 (7)
        Drx Timer Max : 7
        Access Burst Type : 8 bit format shall be used (0)
        Control Ack Type : default format is RLC/MAC control block (1)
        Bs Cv Max : 6
        Pan Dec Included : 1
        Pan Dec : 1
        Pan Inc : 2
        Pan Max : UnKnOwN (4)
        Optional Extension Information Included : 1
        Extension Length : 15
        Egprs Supported Included : 1
        Egprs Packet Channel Request : EGPRS capable MSs shall use two phase packet access with EGPRS PACKET CHANNEL REQUEST message on the PRACH for uplink TBF establishment when there is a PBCCH in cell EGPRS capable MSs shall use two phase packet access with EGPRS PACKET CHANNEL REQUEST message on the RACH when there is no PBCCH in the cell (1)
        Bep Perid : 5
        Pfc Feature Mode : The network supports packet flow context procedures (1)
        Dtm Support : DTM is not supported in the serving cell (0)
        Bss Paging Coordination : The cell does not support Circuit-Switched paging co-ordination (0)
        Ccn Active : 0
        Nw Ext Utbf : 1
        Multiple Tbf Capability : 0
        Spare : 138
      Alpha : 6
      T Avg W : 5
      T Avg T : 1
      Pc Meas Chan : BCCH (0)
      N Avg I : 12