---------------------------------------------------------------------------------------
SYS_Info 1
---------------------------------------------------------------------------------------

GSM RR Signaling Message
  Channel : 129
  Type : 25
  Length : 23
  Direction : Network to UE
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 25 (0x19)
  System Information Type 1
    Cell Channel Description
      GSM Format Id
        Bit Map 0
          CA_ARFCN 124 To 121 : 0x0
          CA_ARFCN 120 To 113 : 0x00
          CA_ARFCN 112 To 105 : 0x00
          CA_ARFCN 104 To 097 : 0x00
          CA_ARFCN 096 To 089 : 0x00
          CA_ARFCN 088 To 081 : 0x00
          CA_ARFCN 080 To 073 : 0x00
          CA_ARFCN 072 To 065 : 0x00
          CA_ARFCN 064 To 057 : 0x00
          CA_ARFCN 056 To 049 : 0x00
          CA_ARFCN 048 To 041 : 0x00
          CA_ARFCN 040 To 033 : 0x00
          CA_ARFCN 032 To 025 : 0x00
          CA_ARFCN 024 To 017 : 0x00
          CA_ARFCN 016 To 009 : 0x00
          CA_ARFCN 008 To 001 : 0x01
    RACH Control Parameter
      Max Retrans : Maximum 4 retransmissions
      Tx Integer : 10 slots used to spread transmission
      Cell Bar Access : The cell is not barred
      RE : Call Reestablishment allowed in the cell
      AC C : 0
    SI 1 Rest Octets
      Band Indicator : 1800 Band


---------------------------------------------------------------------------------------
SYS_Info 2
---------------------------------------------------------------------------------------

GSM RR Signaling Message
  Channel : 129
  Type : 26
  Length : 23
  Direction : Network to UE
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 26 (0x1A)
  System Information Type 2
    BCCH Frequency List
      Bit 128 : 0
      Bit 127 : 0
      Ext Ind : The information element carries the complete BA
      BA Ind : 1
      Bit 124 To 121 : 0x0
      Bit 120 To 113 : 0x00
      Bit 112 To 105 : 0x00
      Bit 104 To 097 : 0x00
      Bit 096 To 089 : 0x00
      Bit 088 To 081 : 0x00
      Bit 080 To 073 : 0x00
      Bit 072 To 065 : 0x00
      Bit 064 To 057 : 0x00
      Bit 056 To 049 : 0x00
      Bit 048 To 041 : 0x00
      Bit 040 To 033 : 0x00
      Bit 032 To 025 : 0x00
      Bit 024 To 017 : 0xE0
      Bit 016 To 009 : 0x00
      Bit 008 To 001 : 0x3F
    NCC Permitted
      NCC Permited : 255
    RACH Control Parameter
      Max Retrans : Maximum 4 retransmissions
      Tx Integer : 10 slots used to spread transmission
      Cell Bar Access : The cell is not barred
      RE : Call Reestablishment allowed in the cell
      AC C : 0


---------------------------------------------------------------------------------------
SYS_Info 2QuaTer
---------------------------------------------------------------------------------------

GSM RR Signaling Message
  Channel : 129
  Type : 7
  Length : 23
  Direction : Network to UE
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 7 (0x7)
  System Information Type 2quater
    SI 2ter Quater Rest Octets
      BA Ind : 1
      3G Ba Ind : 1
      MP Change Mark : 1
      SI2quater Index : 2
      SI2quater Count : 2
      3G CCN Active : 0
      Priority and E-UTRAN Parameters Description
        E-UTRAN Parameters Description
          E-UTRAN CCN Active : 0
          E-UTRAN Start : 0
          E-UTRANStop : 1
          E-UTRAN Neighbour Cells[0]
            EARFCN : 3578
            Measurement Bandwidth : 0
            E-UTRAN_PRIORITY : 5
            THRESH_E-UTRAN_high : 5
            THRESH_E-UTRAN_low : 0
            E-UTRAN_QRXLEVMIN : 6



---------------------------------------------------------------------------------------
SYS_Info 2QuaTer
---------------------------------------------------------------------------------------

GSM RR Signaling Message
  Channel : 129
  Type : 7
  Length : 23
  Direction : Network to UE
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 7 (0x7)
  System Information Type 2quater
    SI 2ter Quater Rest Octets
      BA Ind : 1
      3G Ba Ind : 1
      MP Change Mark : 1
      SI2quater Index : 0
      SI2quater Count : 2
      3G Neighbour Cell Description
        UTRAN FDD Description
          FDD ARFCN : 10564
          FDD Indic0 : 0
          Nr Of FDD Cells : 31
      3G Measurement Parameters Description
        Qsearch I : 7
        Qsearch C Initial : 0
        FDD Qoffset Included : 1
        FDD Qoffset : 0
        FDD Rep Quant : 1
        FDD Multirat Reporting : 2
        FDD Qmin : 7
        TDD Qoffset Included : 0
      3G CCN Active : 0
      Priority and E-UTRAN Parameters Description
        3G Priority Parameters Description
          UTRAN Start : 1
          UTRAN Stop : 1
          Default UTRAN Priority : 4
          Default Thresh UTRAN : 6
          Default UTRAN QrxLevmin : 0



---------------------------------------------------------------------------------------
SYS_Info 2QuaTer
---------------------------------------------------------------------------------------

GSM RR Signaling Message
  Channel : 129
  Type : 7
  Length : 23
  Direction : Network to UE
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 7 (0x7)
  System Information Type 2quater
    SI 2ter Quater Rest Octets
      BA Ind : 1
      3G Ba Ind : 1
      MP Change Mark : 1
      SI2quater Index : 1
      SI2quater Count : 2
      GPRS 3G Measurement Parameters Description
        Qsearch P : 15
        GSM 3g Search Prio : 1
        FDD Rep Quant Included : 0
        FDD Reporting Offset Included : 0
        TDD Multirat Reporting Included : 0
        TDD Reporting Offset Included : 0
      3G Additional Measurement Parameters Description
        FDD Qmin Offset : 0
        FDD RSCP min : 6
      3G Additional Measurement Parameters Description 2
        FDD Reporting Threshold 2 : 11
      3G CCN Active : 0
      Priority and E-UTRAN Parameters Description
        Serving Cell Priority Parameters Description
          GERAN Priority : 2
          Thresh Priority Search : 15
          Thresh GSM Low : 15
          H_PRIO : 0
          T_Reselection : 1
        E-UTRAN Parameters Description
          E-UTRAN CCN Active : 0
          E-UTRAN Start : 1
          E-UTRANStop : 0
          E-UTRAN Measurement Parameters Description
            Qsearch_C_E-UTRAN_Initial : 0
            E-UTRAN_REP_QUANT : 0
            E-UTRAN_MULTIRAT_REPORTING : 0
            REPORTING_GRANULARITY : 0
          E-UTRAN Neighbour Cells[0]
            EARFCN : 103
            Measurement Bandwidth : 0
            E-UTRAN_PRIORITY : 6
            THRESH_E-UTRAN_high : 5
            THRESH_E-UTRAN_low : 0
            E-UTRAN_QRXLEVMIN : 10


---------------------------------------------------------------------------------------
SYS_Info 3
---------------------------------------------------------------------------------------

GSM RR Signaling Message
  Channel : 129
  Type : 27
  Length : 23
  Direction : Network to UE
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 27 (0x1B)
  System Information Type 3
    Cell Identity
      Cell Identity : 52974
    Location Area Identification
      MCC : 226
      MNC : 5
      LAC : 7008
    Control Channel Description
      MSCR : MSC is Release '99 onwards
      ATT : MSs in the cell shall apply IMSI attach and detach procedure
      BS AG BLKS RES : 1
      CCCH CONF : 1 basic physical channel used for CCCH, combined with SDCCHs
      CBQ3 : Iu mode not supported
      BS PA MFRMS : 4 multiframes period for transmission of PAGING REQUEST messages to the same paging subgroup
      T3212 Timeout Value : 30
    Cell Options
      DN-Ind : 0
      PWRC : PWRC is set
      DTX : The MSs shall use uplink discontinuous transmission
      Radio Link Timeout : 4
    Cell Selection Parameters
      Cell Reselect Hysteresis : 4 dB RXLEV hysteresis for LA re-selection
      MS TXPWR MAX CCH : 5
      ACS : System information type 16 and 17 are not broadcast on the BCCH
      NECI : New establishment causes are not supported
      Rxlev Access Min : 0
    RACH Control Parameters
      Max Retrans : Maximum 4 retransmissions
      Tx Integer : 10 slots used to spread transmission
      Cell Bar Access : The cell is not barred
      RE : Call Reestablishment allowed in the cell
      AC C : 0
    SI 3 Rest Octets
      Selection Parameters Included : 0
      Optional Power Offset Included : 0
      System Information 2ter Indicator : SYSTEM INFORMATION TYPE 2ter message is available
      Early Classmark Sending Control : Early Classmark Sending is allowed
      Where Included : 1
      Where : 0
      GPRS Indicator Included : 0
      3G Early Classmark Sending Restriction : Neither UTRAN nor cdma2000 classmark change messages shall be sent with the Early classmark sending
      SI2quater Indicator Included : 1
      SI2quater Position : SYSTEM INFORMATION TYPE 2 quater message is sent on BCCH Norm



---------------------------------------------------------------------------------------
SYS_Info 4
---------------------------------------------------------------------------------------

GSM RR Signaling Message
  Channel : 129
  Type : 28
  Length : 23
  Direction : Network to UE
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 28 (0x1C)
  System Information Type 4
    Location Area Identification
      MCC : 226
      MNC : 5
      LAC : 7008
    Cell Selection Parameters
      Cell Reselect Hysteresis : 4 dB RXLEV hysteresis for LA re-selection
      MS TXPWR MAX CCH : 5
      ACS : System information type 16 and 17 are not broadcast on the BCCH
      NECI : New establishment causes are not supported
      Rxlev Access Min : 0
    RACH Control Parameters
      Max Retrans : Maximum 4 retransmissions
      Tx Integer : 10 slots used to spread transmission
      Cell Bar Access : The cell is not barred
      RE : Call Reestablishment allowed in the cell
      AC C : 0
    CBCH Channel Description
      IEI : 100 (0x64)
      Channel Type : 6
      TN : 0
      TSC : 2
      H : Single RF Channel
      ARFCN : 1
    SI 4 Rest Octets
      SI4 Rest Octets O


---------------------------------------------------------------------------------------
SYS_Info 5
---------------------------------------------------------------------------------------

GSM RR Signaling Message
  Channel : 132
  Type : 29
  Length : 18
  Direction : Network to UE
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 29 (0x1D)
  System Information Type 5
    BCCH Frequency List
      Bit 128 : 0
      Bit 127 : 0
      Ext Ind : The information element carries the complete BA
      BA Ind : 0
      Bit 124 To 121 : 0x0
      Bit 120 To 113 : 0x00
      Bit 112 To 105 : 0x00
      Bit 104 To 097 : 0x00
      Bit 096 To 089 : 0x00
      Bit 088 To 081 : 0x00
      Bit 080 To 073 : 0x00
      Bit 072 To 065 : 0x00
      Bit 064 To 057 : 0x00
      Bit 056 To 049 : 0x00
      Bit 048 To 041 : 0x00
      Bit 040 To 033 : 0x00
      Bit 032 To 025 : 0x00
      Bit 024 To 017 : 0xE0
      Bit 016 To 009 : 0x00
      Bit 008 To 001 : 0x3E




---------------------------------------------------------------------------------------
SYS_Info 6
---------------------------------------------------------------------------------------

GSM RR Signaling Message
  Channel : 132
  Type : 30
  Length : 18
  Direction : Network to UE
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 30 (0x1E)
  System Information Type 6
    Cell Identity
      Cell Identity : 52974
    Location Area Identification
      MCC : 226
      MNC : 5
      LAC : 7008
    Cell Options
      DTX : 0
      PWRC : PWRC is set
      DTX indicator : The MSs shall use uplink discontinuous transmission
      Radio Link Timeout : 4
    NCC Permitted
      NCC Permited : 255
    SI 6 Rest Octets
      DTM Support : 0
      Band Indicator : 1800 Band

