SYSTEM INFORMATION TYPE 1
GSM RR Signaling Message
  Channel : 129
  Type : 25
  Length : 23
  Direction : 0
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 25
  System Information Type 1
    Cell Channel Description
      Gsm Format Id
        Spare : 0
        Bit Map 0
          Caarfcn 124 To 121 : 8
          Caarfcn 120 To 113 : 8
          Caarfcn 112 To 105 : 0
          Caarfcn 104 To 097 : 2
          Caarfcn 096 To 089 : 0
          Caarfcn 088 To 081 : 1
          Caarfcn 080 To 073 : 0
          Caarfcn 072 To 065 : 0
          Caarfcn 064 To 057 : 0
          Caarfcn 056 To 049 : 0
          Caarfcn 048 To 041 : 0
          Caarfcn 040 To 033 : 0
          Caarfcn 032 To 025 : 0
          Caarfcn 024 To 017 : 0
          Caarfcn 016 To 009 : 0
          Caarfcn 008 To 001 : 0
    Rach Control Parameter
      Max Retrans : Maximum 4 retransmissions (2)
      Tx Integer : 32 slots used to spread transmission (14)
      Cell Bar Access : The cell is not barred (0)
      Re : Call Reestablishment not allowed in the cell (1)
      Ac C : 0
    Si 1 Rest Octets
      Band Indicator : 1800 Band (0)

SYSTEM INFORMATION TYPE 2
GSM RR Signaling Message
  Channel : 129
  Type : 26
  Length : 23
  Direction : 0
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 26
  System Information Type 2
    Bcch Frequency List
      Bit 128 : 0
      Bit 127 : 0
      Ext Ind : The information element carries the complete BA (0)
      Ba Ind : 0
      Bit 124 To 121 : 0
      Bit 120 To 113 : 0
      Bit 112 To 105 : 0
      Bit 104 To 097 : 0
      Bit 096 To 089 : 1
      Bit 088 To 081 : 247
      Bit 080 To 073 : 248
      Bit 072 To 065 : 0
      Bit 064 To 057 : 0
      Bit 056 To 049 : 0
      Bit 048 To 041 : 0
      Bit 040 To 033 : 0
      Bit 032 To 025 : 0
      Bit 024 To 017 : 0
      Bit 016 To 009 : 0
      Bit 008 To 001 : 0
    Ncc Permitted
      Ncc Permited : 255
    Rach Control Parameter
      Max Retrans : Maximum 4 retransmissions (2)
      Tx Integer : 32 slots used to spread transmission (14)
      Cell Bar Access : The cell is not barred (0)
      Re : Call Reestablishment not allowed in the cell (1)
      Ac C : 0

SYSTEM INFORMATION TYPE 2 QuaTer
GSM RR Signaling Message
  Channel : 129
  Type : 7
  Length : 23
  Direction : 0
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 7
  System Information Type 2quater
    Si 2ter Quater Rest Octets
      Ba Ind : 0
      3g Ba Ind : 1
      Mp Change Mark : 1
      Si2quater Index : 1
      Si2quater Count : 4
      3G Neighbour Cell Description
        Index Start 3g : 0
        UTRAN FDD Description
          FDD ARFCN : 10713
          FDD Indic0 : 0
          Nr Of Fdd Cells : 4
          W : 56
          W : 511
          W : 331
          W : 255

SYSTEM INFORMATION TYPE 2 QuaTer
GSM RR Signaling Message
  Channel : 129
  Type : 7
  Length : 23
  Direction : 0
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 7
  System Information Type 2quater
    Si 2ter Quater Rest Octets
      Ba Ind : 0
      3g Ba Ind : 1
      Mp Change Mark : 1
      Si2quater Index : 0
      Si2quater Count : 4
      Measurement Parameters Description
        Report Type : 1
        Serving Band Reporting : 3
      GPRS Measurement Parameters Description
        Report Type : 1
        Reporting Rate : 0
        Invalid Bsic Reporting : 0
        Multiband Reporting : 2
        Serving Band Reporting : 3
        Scale Ord : 0
        Gsm 900 Reporting Band Offset : 0
        Gsm 900 Reporting Band Threshold : 0
        Gsm 1800 Reporting Band Offset : 0
        Gsm 1800 Reporting Band Threshold : 0
      NC Measurement Parameters
        Network Control Order : 0
        Nc Reporting Drx Period Included : 1
        Nc Reporting Drx Period : 1
        Nc Reporting Period I : 5
        Nc Reporting Period T : 1
      3G Measurement Parameters Description
        Qsearch I : 7
        Qsearch C Initial : 0
        Fdd Qoffset Included : 1
        Fdd Qoffset : 0
        Fdd Rep Quant : 0
        Fdd Multirat Reporting : 2
        Fdd Qmin : 7
        Tdd Qoffset Included : 0
      GPRS 3G Measurement Parameters Description
        Qsearch P : 7
        Gsm 3g Search Prio : 1
        Fdd Rep Quant Included : 1
        Fdd Rep Quant : 0
        Fdd Multirat Reporting : 2
        Fdd Reporting Offset Included : 1
        Fdd Reporting Offset : 0
        Fdd Reporting Threshold : 0
        Tdd Multirat Reporting Included : 0
        Tdd Reporting Offset Included : 0

SYSTEM INFORMATION TYPE 2 QuaTer
GSM RR Signaling Message
  Channel : 129
  Type : 7
  Length : 23
  Direction : 0
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 7
  System Information Type 2quater
    Si 2ter Quater Rest Octets
      Ba Ind : 0
      3g Ba Ind : 1
      Mp Change Mark : 1
      Si2quater Index : 2
      Si2quater Count : 4
      3G Neighbour Cell Description
        Index Start 3g : 4
        UTRAN FDD Description
          FDD ARFCN : 10738
          FDD Indic0 : 0
          Nr Of Fdd Cells : 3
          W : 307
          W : 480
          W : 47
      3G Additional Measurement Parameters Description
        FDD Qmin Offset : 0
        FDD RSCP min : 3

SYSTEM INFORMATION TYPE 2 QuaTer
GSM RR Signaling Message
  Channel : 129
  Type : 7
  Length : 23
  Direction : 0
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 7
  System Information Type 2quater
    Si 2ter Quater Rest Octets
      Ba Ind : 0
      3g Ba Ind : 1
      Mp Change Mark : 1
      Si2quater Index : 3
      Si2quater Count : 4
      3G CCN Active : 1
      Priority and E-UTRAN Parameters Description
        Serving Cell Priority Parameters Description
          Geran Priority : 4
          Thresh Priority Search : 15
          Thresh GSM Low : 0
          H_PRIO : 0
          T_Reselection : 0
        3G Priority Parameters Description
          Utran Start : 0
          Utran Stop : 0
          Default Utran Priority : 6
          Default Thresh Utran : 4
          Default Utran QrxLevmin : 2
          Repeated UTRAN Priority Parameters[0]
            UTRAN Frequency Index : 0
            UTRAN Frequency Index : 1
          Repeated UTRAN Priority Parameters[1]
            Thresh UTRAN Low : 20
        E-UTRAN Parameters Description
          E-Utran CCN Active : 1
          E-Utran Start : 1
          E-Utran Stop : 0
          E-UTRAN Measurement Parameters Description
            Qsearch_C_E-UTRAN_Initial : 15
            E-UTRAN_REP_QUANT : 0
            E-UTRAN_MULTIRAT_REPORTING : 2
            E-UTRAN_FDD_REPORTING_THRESHOLD : 0
          GPRS E-UTRAN Measurement Parameters Description
            Qsearch_P_E-UTRAN : 15
            E-UTRAN_REP_QUANT : 0
            E-UTRAN_MULTIRAT_REPORTING : 2
            E-UTRAN_FDD_REPORTING_THRESHOLD : 0

SYSTEM INFORMATION TYPE 2 QuaTer
GSM RR Signaling Message
  Channel : 129
  Type : 7
  Length : 23
  Direction : 0
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 7
  System Information Type 2quater
    Si 2ter Quater Rest Octets
      Ba Ind : 0
      3g Ba Ind : 1
      Mp Change Mark : 1
      Si2quater Index : 4
      Si2quater Count : 4
      3G CCN Active : 1
      Priority and E-UTRAN Parameters Description
        E-UTRAN Parameters Description
          E-Utran CCN Active : 1
          E-Utran Start : 0
          E-Utran Stop : 1
          E-UTRAN Neighbour Cells[0]
            EARFCN : 6350
            E-UTRAN_PRIORITY : 7
            THRESH_E-UTRAN_high : 9
            THRESH_E-UTRAN_low : 20
            E-UTRAN_QRXLEVMIN : 6

SYSTEM INFORMATION TYPE 3
GSM RR Signaling Message
  Channel : 129
  Type : 27
  Length : 23
  Direction : 0
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 27
  System Information Type 3
    Cell Identity : 32305
    Location Area Identification
      MCC : 226
      MNC : 10
      LAC : 16105
    Control Channel Description
      Mscr : MSC is Release '99 onwards (1)
      Att : MSs in the cell shall apply IMSI attach and detach procedure (1)
      Bs Ag Blks Res : 3
      Ccch Conf : 1 basic physical channel used for CCCH, not combined with SDCCHs (0)
      Spare : 0
      Cbq3 : Iu mode not supported (0)
      Spare : 0
      Bs Pa Mfrms : UnKnOwN (3)
      T3212 Timeout Value : UnKnOwN (40)
    Cell Options
      Dn-Ind : 0
      Pwrc : PWRC is set (1)
      Dtx : The MSs shall use uplink discontinuous transmission (1)
      Radio Link Timeout : 5
    Cell Selection Parameters
      Cell Reselect Hysteresis : 8 dB RXLEV hysteresis for LA re-selection (4)
      Ms Txpwr Max Cch : 5
      Acs : System information type 16 and 17 are not broadcast on the BCCH (0)
      Neci : New establishment causes are supported (1)
      Rxlev Access Min : 2
    Rach Control Parameters
      Max Retrans : Maximum 4 retransmissions (2)
      Tx Integer : 32 slots used to spread transmission (14)
      Cell Bar Access : The cell is not barred (0)
      Re : Call Reestablishment not allowed in the cell (1)
      Ac C : 0
    Si 3 Rest Octets
      Selection Parameters Included : 0
      Optional Power Offset Included : 1
      Power Offset : 1
      System Information 2ter Indicator : SYSTEM INFORMATION TYPE 2ter message is available (1)
      Early Classmark Sending Control : Early Classmark Sending is allowed (1)
      Where Included : 1
      Where : 0
      Gprs Indicator Included : 1
      Ra Colour : 1
      Si13 Position : SYSTEM INFORMATION TYPE 13 message is sent on BCCH Norm (0)
      3g Early Classmark Sending Restriction : The sending of UTRAN and CDMA2000 Classmark Sending messages is controlled by the Early Classmark Sending Control parameter (1)
      Si2quater Indicator Included : 0

SYSTEM INFORMATION TYPE 4
GSM RR Signaling Message
  Channel : 129
  Type : 28
  Length : 23
  Direction : 0
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 28
  System Information Type 4
    Location Area Identification
      MCC : 226
      MNC : 10
      LAC : 16105
    Cell Selection Parameters
      Cell Reselect Hysteresis : 8 dB RXLEV hysteresis for LA re-selection (4)
      Ms Txpwr Max Cch : 5
      Acs : System information type 16 and 17 are not broadcast on the BCCH (0)
      Neci : New establishment causes are supported (1)
      Rxlev Access Min : 2
    Rach Control Parameters
      Max Retrans : Maximum 4 retransmissions (2)
      Tx Integer : 32 slots used to spread transmission (14)
      Cell Bar Access : The cell is not barred (0)
      Re : Call Reestablishment not allowed in the cell (1)
      Ac C : 0
    Cbch Channel Description
      Channel Type : 10
      Tn : 1
      Tsc : 3
      H : RF hopping Channel (1)
      Maio : 0
      Hsn : 39
    Cbch Mobile Allocation
      Length : 1
      Ma C (Octet) : 15
    Si 4 Rest Octets
      Si4 Rest Octets O
        Power Offset : 1
        Ra Colour : 1
        SI13 Position : 0

SYSTEM INFORMATION TYPE 5
GSM RR Signaling Message
  Channel : 132
  Type : 29
  Length : 18
  Direction : 0
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 29
  System Information Type 5
    Bcch Frequency List
      Bit 128 : 0
      Bit 127 : 0
      Ext Ind : The information element carries the complete BA (0)
      Ba Ind : 0
      Bit 124 To 121 : 0
      Bit 120 To 113 : 0
      Bit 112 To 105 : 0
      Bit 104 To 097 : 0
      Bit 096 To 089 : 1
      Bit 088 To 081 : 247
      Bit 080 To 073 : 248
      Bit 072 To 065 : 0
      Bit 064 To 057 : 0
      Bit 056 To 049 : 0
      Bit 048 To 041 : 0
      Bit 040 To 033 : 0
      Bit 032 To 025 : 0
      Bit 024 To 017 : 0
      Bit 016 To 009 : 0
      Bit 008 To 001 : 0

SYSTEM INFORMATION TYPE 13
GSM RR Signaling Message
  Channel : 129
  Type : 0
  Length : 23
  Direction : 0
  Skip indicator : 0
  Protocol Discriminator : 6
  Message ID : 0
  System Information Type 13
    Si 13 Rest Octets
      BCCH Change Mark : 2
      Si Change Field : Update of unspecified SI message or SI messages (0)
      RAC : 161
      SPGC CCCH Sup : 0
      Priority Access Thr : 6
      Network Control Order : 0
      GPRS Cell Options
        Nmo : Network Mode of Operation II (1)
        T3168 : 3
        T3192 : 500 (0)
        Drx Timer Max : 3
        Access Burst Type : 8 bit format shall be used (0)
        Control Ack Type : default format is four access bursts (0)
        Bs Cv Max : 12
        Pan Dec Included : 1
        Pan Dec : 1
        Pan Inc : 2
        Pan Max : UnKnOwN (4)
        Optional Extension Information Included : 1
        Extension Length : 10
        Egprs Supported Included : 1
        Egprs Packet Channel Request : EGPRS capable MSs shall use EGPRS PACKET CHANNEL REQUEST message for uplink TBF establishment on the PRACH when there is a PBCCH in cell or on the RACH when there is no PBCCH in the cell (0)
        Bep Perid : 5
        Pfc Feature Mode : The network does not support packet flow context procedures (0)
        Dtm Support : DTM is not supported in the serving cell (0)
        Bss Paging Coordination : The cell does not support Circuit-Switched paging co-ordination (0)
        Ccn Active : 1
        Nw Ext Utbf : 1
        Multiple Tbf Capability : 0
        Spare : 20
      Alpha : 6
      T Avg W : 9
      T Avg T : 13
      Pc Meas Chan : PDCH (1)
      N Avg I : 6