MASTER INFORMATION BLOCK
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 19
  mib
    mib-ValueTag : 7
    plmn-Type
      gsm-MAP
        plmn-Identity
          mcc
            MCC[0]
              Digit : 2
            MCC[1]
              Digit : 2
            MCC[2]
              Digit : 6
          mnc
            MNC[0]
              Digit : 0
            MNC[1]
              Digit : 5
    sibSb-ReferenceList
      SIBSb-ReferenceList[0]
        sibSb-Type
          sysInfoTypeSB1 : 3
        scheduling
          scheduling
            sib-Pos
              rep8 : 1
      SIBSb-ReferenceList[1]
        sibSb-Type
          sysInfoType5 : 3
        scheduling
          scheduling
            segCount : 3
            sib-Pos
              rep32 : 2
            sib-PosOffsetInfo
              SibOFF-List[0]
                SibOFF : so2
              SibOFF-List[1]
                SibOFF : so6
      SIBSb-ReferenceList[2]
        sibSb-Type
        scheduling
          scheduling
            sib-Pos
              rep8 : 1
      SIBSb-ReferenceList[3]
        sibSb-Type
          sysInfoType11 : 3
        scheduling
          scheduling
            segCount : 6
            sib-Pos
              rep64 : 11
            sib-PosOffsetInfo
              SibOFF-List[0]
                SibOFF : so6
              SibOFF-List[1]
                SibOFF : so2
              SibOFF-List[2]
                SibOFF : so24
              SibOFF-List[3]
                SibOFF : so6
              SibOFF-List[4]
                SibOFF : so2

SYS.INFO.TYPE SB1
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 13
  sysInfoSB1
    sib-ReferenceList
      SIB-ReferenceList[0]
        sib-Type
          sysInfoType1 : 207
        scheduling
          scheduling
            sib-Pos
              rep64 : 23
      SIB-ReferenceList[1]
        sib-Type
          sysInfoType2 : 3
        scheduling
          scheduling
            sib-Pos
              rep8 : 1
      SIB-ReferenceList[2]
        sib-Type
          sysInfoType3 : 3
        scheduling
          scheduling
            sib-Pos
              rep64 : 10
    v6b0NonCriticalExtensions
      sysInfoTypeSB1-v6b0ext
      v860NonCriticalExtensions
        sysInfoTypeSB1-v860ext
          extSIBTypeInfoSchedulingInfo-List
            ExtSIBTypeInfoSchedulingInfo-List2[0]
              extensionSIB-Type2
              schedulingInfo
                scheduling
                  sib-Pos
                    rep64 : 7
              valueTagInfo
                cellValueTag : 3

SYS.INFO.TYPE 1
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 20
  sysInfoType1
    cn-CommonGSM-MAP-NAS-SysInfo : '02C3'H (707)
    cn-DomainSysInfoList
      CN-DomainSysInfoList[0]
        cn-DomainIdentity : cs-domain
        cn-Type
          gsm-MAP : '1E01'H (7681)
        cn-DRX-CycleLengthCoeff : 6
      CN-DomainSysInfoList[1]
        cn-DomainIdentity : ps-domain
        cn-Type
          gsm-MAP : '6B01'H (27393)
        cn-DRX-CycleLengthCoeff : 6
    ue-ConnTimersAndConstants
      t-302 : ms1600
      n-304 : 3
      t-307 : s50
      t-308 : ms40
      t-309 : 8
      t-310 : ms40
      n-310 : 0
      t-311 : ms250
      t-314 : s20
      t-315 : s30
      t-317 : infinity2
    ue-IdleTimersAndConstants
      t-300 : ms2000
      n-300 : 3
      t-312 : 6
      n-312 : s1
    v3a0NonCriticalExtensions
      sysInfoType1-v3a0ext
        ue-ConnTimersAndConstants-v3a0ext
          n-315 : s20
        ue-IdleTimersAndConstants-v3a0ext
          n-312 : s4
      v860NonCriticalExtentions
        sysInfoType1-v860ext
          ue-ConnTimersAndConstants
            t-323 : s5

SYS.INFO.TYPE 2
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 4
  sysInfoType2
    ura-IdentityList
      URA-IdentityList[0]
        URA-Identity : '0001'H (1)

SYS.INFO.TYPE 3
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 18
  sysInfoType3
    sib4indicator : false
    cellIdentity : '2BECEEB'H (46059243)
    cellSelectReselectInfo
      cellSelectQualityMeasure
        cpich-Ec-N0
          q-HYST-2-S : 1
      modeSpecificInfo
        fdd
          s-Intrasearch : 5
          s-Intersearch : 3
          rat-List
            RAT-FDD-InfoList[0]
              rat-Identifier : gsm
              s-SearchRAT : 2
              s-Limit-SearchRAT : 0
          q-QualMin : -18
          q-RxlevMin : -58
      q-Hyst-l-S : 2
      t-Reselection-S : 1
      maxAllowedUL-TX-Power : 21
    cellAccessRestriction
      cellBarred
      cellReservedForOperatorUse : notReserved
      cellReservationExtension : notReserved
      accessClassBarredList
        AccessClassBarredList[0]
          AccessClassBarred : notBarred
        AccessClassBarredList[1]
          AccessClassBarred : notBarred
        AccessClassBarredList[2]
          AccessClassBarred : notBarred
        AccessClassBarredList[3]
          AccessClassBarred : notBarred
        AccessClassBarredList[4]
          AccessClassBarred : notBarred
        AccessClassBarredList[5]
          AccessClassBarred : notBarred
        AccessClassBarredList[6]
          AccessClassBarred : notBarred
        AccessClassBarredList[7]
          AccessClassBarred : notBarred
        AccessClassBarredList[8]
          AccessClassBarred : notBarred
        AccessClassBarredList[9]
          AccessClassBarred : notBarred
        AccessClassBarredList[10]
          AccessClassBarred : notBarred
        AccessClassBarredList[11]
          AccessClassBarred : notBarred
        AccessClassBarredList[12]
          AccessClassBarred : notBarred
        AccessClassBarredList[13]
          AccessClassBarred : notBarred
        AccessClassBarredList[14]
          AccessClassBarred : notBarred
        AccessClassBarredList[15]
          AccessClassBarred : notBarred
    v4b0NonCriticalExtensions
      sysInfoType3-v4b0ext
      v590NonCriticalExtension
        sysInfoType3-v590ext
        v5c0NoncriticalExtension
          sysInfoType3-v5c0ext
          v670NonCriticalExtension
            sysInfoType3-v670ext
              domainSpecificAccessRestrictionParametersForPLMNOfMIB
                cSDomainSpecificAccessRestriction
                pSDomainSpecificAccessRestriction

SYS.INFO.TYPE 5
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 69
  sysInfoType5
    sib6indicator : false
    pich-PowerOffset : -7
    modeSpecificInfo
      fdd
        aich-PowerOffset : -6
    primaryCCPCH-Info
      fdd
        tx-DiversityIndicator : false
    prach-SystemInformationList
      PRACH-SystemInformationList[0]
        prach-RACH-Info
          modeSpecificInfo
            fdd
              availableSignatures : '00FF'H (255)
              availableSF : sfpr32
              preambleScramblingCodeWordNumber : 0
              puncturingLimit : pl1
              availableSubChannelNumbers : 'FFF'H (4095)
        transportChannelIdentity : 1
        rach-TransportFormatSet
          commonTransChTFS
            tti
              tti20
                CommonDynamicTF-InfoList[0]
                  rlc-Size
                    fdd
                      octetModeRLC-SizeInfoType2
                        sizeType1 : 15
                  numberOfTbSizeList[0]
                  logicalChannelList
                CommonDynamicTF-InfoList[1]
                  rlc-Size
                    fdd
                      octetModeRLC-SizeInfoType2
                        sizeType2 : 3
                  numberOfTbSizeList[0]
                  logicalChannelList
            semistaticTF-Information
              channelCodingType
                convolutional : half
              rateMatchingAttribute : 1
              crc-Size : crc16
        rach-TFCS
          normalTFCI-Signalling
            complete
              ctfcSize
                ctfc2Bit[0]
                  ctfc2 : 0
                  powerOffsetInformation
                    gainFactorInformation
                      signalledGainFactors
                        modeSpecificInfo
                          fdd
                            gainFactorBetaC : 13
                        gainFactorBetaD : 15
                    powerOffsetPp-m : -3
                ctfc2Bit[1]
                  ctfc2 : 1
                  powerOffsetInformation
                    gainFactorInformation
                      signalledGainFactors
                        modeSpecificInfo
                          fdd
                            gainFactorBetaC : 10
                        gainFactorBetaD : 15
                    powerOffsetPp-m : -2
        prach-Partitioning
          fdd[0]
            accessServiceClass-FDD
              availableSignatureStartIndex : 0
              availableSignatureEndIndex : 7
              assignedSubChannelNumber : 'F'H (15)
        ac-To-ASC-MappingTable
          AC-To-ASC-MappingTable[0]
            AC-To-ASC-Mapping : 0
          AC-To-ASC-MappingTable[1]
            AC-To-ASC-Mapping : 0
          AC-To-ASC-MappingTable[2]
            AC-To-ASC-Mapping : 0
          AC-To-ASC-MappingTable[3]
            AC-To-ASC-Mapping : 0
          AC-To-ASC-MappingTable[4]
            AC-To-ASC-Mapping : 0
          AC-To-ASC-MappingTable[5]
            AC-To-ASC-Mapping : 0
          AC-To-ASC-MappingTable[6]
            AC-To-ASC-Mapping : 0
        modeSpecificInfo
          fdd
            primaryCPICH-TX-Power : 33
            constantValue : -20
            prach-PowerOffset
              powerRampStep : 2
              preambleRetransMax : 20
            rach-TransmissionParameters
              mmax : 8
              nb01Min : 0
              nb01Max : 0
            aich-Info
              channelisationCode256 : 2
              sttd-Indicator : false
              aich-TransmissionTiming : e1
    sCCPCH-SystemInformationList
      SCCPCH-SystemInformationList[0]
        secondaryCCPCH-Info
          modeSpecificInfo
            fdd
              dummy1 : mayBeUsed
              sttd-Indicator : false
              sf-AndCodeNumber
                sf64 : 1
              pilotSymbolExistence : false
              tfci-Existence : true
              positionFixedOrFlexible : flexible
              timingOffset : 50
        tfcs
          normalTFCI-Signalling
            complete
              ctfcSize
                ctfc4Bit[0]
                  ctfc4 : 0
                ctfc4Bit[1]
                  ctfc4 : 1
                ctfc4Bit[2]
                  ctfc4 : 2
                ctfc4Bit[3]
                  ctfc4 : 3
                ctfc4Bit[4]
                  ctfc4 : 4
                ctfc4Bit[5]
                  ctfc4 : 6
        fach-PCH-InformationList
          FACH-PCH-InformationList[0]
            transportFormatSet
              commonTransChTFS
                tti
                  tti10
                    CommonDynamicTF-InfoList[0]
                      rlc-Size
                        fdd
                          octetModeRLC-SizeInfoType2
                            sizeType1 : 24
                      numberOfTbSizeList[0]
                      numberOfTbSizeList[1]
                      logicalChannelList
                semistaticTF-Information
                  channelCodingType
                    convolutional : half
                  rateMatchingAttribute : 230
                  crc-Size : crc16
            transportChannelIdentity : 3
            ctch-Indicator : false
          FACH-PCH-InformationList[1]
            transportFormatSet
              commonTransChTFS
                tti
                  tti10
                    CommonDynamicTF-InfoList[0]
                      rlc-Size
                        fdd
                          octetModeRLC-SizeInfoType2
                            sizeType1 : 15
                      numberOfTbSizeList[0]
                      numberOfTbSizeList[1]
                      numberOfTbSizeList[2]
                        small : 2
                      logicalChannelList
                semistaticTF-Information
                  channelCodingType
                    convolutional : half
                  rateMatchingAttribute : 220
                  crc-Size : crc16
            transportChannelIdentity : 4
            ctch-Indicator : false
          FACH-PCH-InformationList[2]
            transportFormatSet
              commonTransChTFS
                tti
                  tti10
                    CommonDynamicTF-InfoList[0]
                      rlc-Size
                        fdd
                          octetModeRLC-SizeInfoType2
                            sizeType2 : 3
                      numberOfTbSizeList[0]
                      numberOfTbSizeList[1]
                      logicalChannelList
                semistaticTF-Information
                  channelCodingType
                  rateMatchingAttribute : 130
                  crc-Size : crc16
            transportChannelIdentity : 5
            ctch-Indicator : false
        pich-Info
          fdd
            channelisationCode256 : 3
            pi-CountPerFrame : e36
            sttd-Indicator : false
    v4b0NonCriticalExtensions
      sysInfoType5-v4b0ext
        frequencyBandIndicator : extension-indicator
      v590NonCriticalExtensions
        v650NonCriticalExtensions
          sysInfoType5-v650ext
            frequencyBandIndicator2 : bandVIII
          v680NonCriticalExtensions
            sysInfoType5-v680ext
              hsdpa-CellIndicator : hsdpa-CapableCell
            v690NonCriticalExtensions
              sysInfoType5-v690ext
                edch-CellIndicator : edch-CapableCell

SYS.INFO.TYPE 7
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 4
  sysInfoType7
    modeSpecificInfo
      fdd
        ul-Interference : -105
    prach-Information-SIB5-List
      DynamicPersistenceLevelList[0]
        DynamicPersistenceLevel : 1

SYS.INFO.TYPE 11
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 165
  sysInfoType11
    sib12indicator : false
    fach-MeasurementOccasionInfo
      fACH-meas-occasion-coeff : 3
      inter-freq-FDD-meas-ind : true
      inter-freq-TDD-meas-ind : false
    measurementControlSysInfo
      use-of-HCS
        hcs-not-used
          cellSelectQualityMeasure
            cpich-Ec-N0
              intraFreqMeasurementSysInfo
                intraFreqCellInfoSI-List
                  removedIntraFreqCellList
                  newIntraFreqCellList
                    NewIntraFreqCellSI-List-ECN0[0]
                      intraFreqCellID : 0
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 124
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[1]
                      intraFreqCellID : 1
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 189
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[2]
                      intraFreqCellID : 2
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 163
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[3]
                      intraFreqCellID : 3
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 262
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[4]
                      intraFreqCellID : 4
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 384
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[5]
                      intraFreqCellID : 5
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 373
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[6]
                      intraFreqCellID : 6
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 333
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[7]
                      intraFreqCellID : 7
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 287
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[8]
                      intraFreqCellID : 8
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 303
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[9]
                      intraFreqCellID : 9
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 326
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[10]
                      intraFreqCellID : 10
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 192
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[11]
                      intraFreqCellID : 11
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 372
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[12]
                      intraFreqCellID : 12
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 338
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[13]
                      intraFreqCellID : 13
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 376
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[14]
                      intraFreqCellID : 14
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 149
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[15]
                      intraFreqCellID : 15
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 39
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[16]
                      intraFreqCellID : 16
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 184
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[17]
                      intraFreqCellID : 17
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 398
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[18]
                      intraFreqCellID : 18
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 375
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[19]
                      intraFreqCellID : 19
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 300
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[20]
                      intraFreqCellID : 20
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 135
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[21]
                      intraFreqCellID : 21
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 218
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[22]
                      intraFreqCellID : 22
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 474
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[23]
                      intraFreqCellID : 23
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 429
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[24]
                      intraFreqCellID : 24
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 332
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[25]
                      intraFreqCellID : 25
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 346
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[26]
                      intraFreqCellID : 26
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 364
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[27]
                      intraFreqCellID : 27
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 288
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[28]
                      intraFreqCellID : 28
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 480
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[29]
                      intraFreqCellID : 29
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 231
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false

                intraFreqReportingQuantityForRACH
                  sfn-SFN-OTD-Type : noReport
                  modeSpecificInfo
                    fdd
                      intraFreqRepQuantityRACH-FDD : cpich-EcN0
                maxReportedCellsOnRACH : currentAnd-2-BestNeighbour
              interFreqMeasurementSysInfo
                interFreqCellInfoSI-List
                  removedInterFreqCellList
                  newInterFreqCellList
                    NewInterFreqCellSI-List-ECN0[0]
                      interFreqCellID : 0
                      frequencyInfo
                        modeSpecificInfo
                          fdd
                            uarfcn-UL : 9614
                            uarfcn-DL : 10564
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 184
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[1]
                      interFreqCellID : 1
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 44
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[2]
                      interFreqCellID : 2
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 263
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[3]
                      interFreqCellID : 3
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 474
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[4]
                      interFreqCellID : 4
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 204
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                        cellSelectionReselectionInfo
                          maxAllowedUL-TX-Power : 24
                          modeSpecificInfo
                            fdd
                    NewInterFreqCellSI-List-ECN0[5]
                      interFreqCellID : 5
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 280
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                        cellSelectionReselectionInfo
                          maxAllowedUL-TX-Power : 24
                          modeSpecificInfo
                            fdd
                    NewInterFreqCellSI-List-ECN0[6]
                      interFreqCellID : 6
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 31
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                        cellSelectionReselectionInfo
                          maxAllowedUL-TX-Power : 24
                          modeSpecificInfo
                            fdd
                    NewInterFreqCellSI-List-ECN0[7]
                      interFreqCellID : 7
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 155
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                        cellSelectionReselectionInfo
                          maxAllowedUL-TX-Power : 24
                          modeSpecificInfo
                            fdd
                    NewInterFreqCellSI-List-ECN0[8]
                      interFreqCellID : 8
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 350
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[9]
                      interFreqCellID : 9
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 53
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[10]
                      interFreqCellID : 10
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 39
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[11]
                      interFreqCellID : 11
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 369
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[12]
                      interFreqCellID : 12
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 131
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[13]
                      interFreqCellID : 13
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 405
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[14]
                      interFreqCellID : 14
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 157
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[15]
                      interFreqCellID : 15
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 117
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[16]
                      interFreqCellID : 16
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 139
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[17]
                      interFreqCellID : 17
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 296
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[18]
                      interFreqCellID : 18
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 289
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[19]
                      interFreqCellID : 19
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 509
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false

SYS.INFO.TYPE 19
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 20
  sysInfoType19
    utra-PriorityInfoList
      utra-ServingCell
        priority : 3
        s-PrioritySearch1 : 2
        s-PrioritySearch2 : 2
        threshServingLow : 1
      utran-FDD-FrequencyList
        UTRAN-FDD-FrequencyList[0]
          uarfcn : 10564
          priority : 4
          threshXhigh : 0
          threshXlow : 0
          qQualMinFDD : -18
          qRxLevMinFDD : -58
    eutra-FrequencyAndPriorityInfoList
      EUTRA-FrequencyAndPriorityInfoList[0]
        earfcn : 103
        measurementBandwidth : mbw50
        priority : 6
        qRxLevMinEUTRA : -64
        threshXhigh : 9
        threshXlow : 2
        eutraDetection : true
      EUTRA-FrequencyAndPriorityInfoList[1]
        earfcn : 37950
        measurementBandwidth : mbw100
        priority : 7
        qRxLevMinEUTRA : -64
        threshXhigh : 9
        threshXlow : 10
        eutraDetection : true

————————————————————————————————
BlackBerry 9720
————————————————————————————————

CELL INFORMATION

3G NS noPDP IDLE
RRC State: IDLE

PSC=124 UARFCN=(8)2988 RSSI=-55
MCC: 226  MNC:5f LAC: 02c3 RAC:006b
NCO: 0  NMO: 1
MSC Rev: 99+ SGSN Rev: 99+

URA_ID: later
DRX Cycle Length: 64

SIB VALIDITY

Uarfcn = 2988 and Psc = 124
MIB validity = Valid
SIB1 validity = Valid
SIB2 validity = Valid
SIB3 validity = Valid
SIB4 validity = Invalid
SIB5 validity = Valid
SIB6 validity = Invalid
SIB7 validity = Invalid
SIB11 validity = Valid
SIB12 validity = Invalid
SIB13 validity = Invalid
SIB13.1 validity = Invalid
SIB13.2 validity = Invalid
SIB13.3 validity = Invalid
SIB13.4 validity = Invalid
SIB14 validity = Invalid
SIB15 validity = Invalid
SIB15.1 validity = Invalid
SIB15.2 validity = Invalid
SIB15.3 validity = Invalid
SIB16 validity = Invalid
SIB17 validity = Invalid
SIB15.4 validity = Invalid
SIB18 validity = Invalid
SB1 validity = Valid
SB2 validity = Invalid
SIB15.5 validity = Invalid

MIB

MIB Value Tag: 7
MCC:2 2 6  MNC:0  d 5 
SIB1 not scheduled in MIB
SIB2 not scheduled in MIB
SIB3 not scheduled in MIB
SIB4 not scheduled in MIB
SIB5 scheduled with tag 3
SIB6 not scheduled in MIB
SIB7 scheduled with tag 0
SIB11 scheduled with tag 3
SIB12 not scheduled in MIB
SIB13 not scheduled in MIB
SIB13.1 not scheduled in MIB
SIB13.2 not scheduled in MIB
SIB13.3 not scheduled in MIB
SIB13.4 not scheduled in MIB
SIB14 not scheduled in MIB
SIB15 not scheduled in MIB
SIB16 not scheduled in MIB
SIB17 not scheduled in MIB
SB1 scheduled with tag 3
SB2 not scheduled in MIB
SIB15.1 not scheduled in MIB
SIB15.2 not scheduled in MIB
SIB15.2 not scheduled in MIB
SIB15.4 not scheduled in MIB
SIB18 not scheduled in MIB
SIB15.5 not scheduled in MIB

SCHEDULING BLK 1

SIB1 scheduled with tag 207
SIB2 scheduled with tag 3
SIB3 scheduled with tag 3
SIB4 not scheduled in sb1
SIB5 not scheduled in sb1
SIB6 not scheduled in sb1
SIB7 not scheduled in sb1
SIB11 not scheduled in sb1
SIB12 not scheduled in sb1
SIB13 not scheduled in sb1
SIB13.1 not scheduled in sb1
SIB13.2 not scheduled in sb1
SIB13.3 not scheduled in sb1
SIB13.4 not scheduled in sb1
SIB14 not scheduled in sb1
SIB15 not scheduled in sb1
SIB16 not scheduled in sb1
SIB17 not scheduled in sb1
SB1 not scheduled in sb1
sb1 not scheduled in sb1
SIB15.1 not scheduled in sb1
SIB15.2 not scheduled in sb1
SIB15.2 not scheduled in sb1
SIB15.4 not scheduled in sb1
SIB18 not scheduled in sb1
SIB15.5 not scheduled in sb1

SB 2 not present

SIB 1

T300: 2000
N300: 3
T302: 1600
N302: 3
T323: 5

SIB 2

Number of UraId: 1
UraId1 = 1:
UraId2 Absent
UraId3 Absent
UraId4 Absent
UraId5 Absent
UraId6 Absent
UraId7 Absent
UraId8 Absent

SIB 3

Cell Identity: 46059243
Sib4Indicator: False
Barred Status: Not Barred
Reserve Indicator: Not reserved
Access Barred list: Present
AccessBarredClassBitmap: 0
Cell Sel Critieria: CPICH-Ec/No
Qqualmin: -18
QrxlevMin: -58
Max UL TX Power: 21
s_IntraSearch: 10
s_InterSearch: 6
s_SearchHCS: INVALID
s_HCS_GSM: INVALID
s_Limit_SearchRAT: 0

SIB 5

Sib6Indicator: False
Total Prach Config: 1
Step:2 RetranMax:20 mMax:8
PrachConfig2 Absent
PrachConfig3 Absent
PrachConfig4 Absent
PrachConfig5 Absent
PrachConfig6 Absent
PrachConfig7 Absent
PrachConfig8 Absent
PrachConfig9 Absent
PrachConfig10 Absent
PrachConfig11 Absent
PrachConfig12 Absent
PrachConfig13 Absent
PrachConfig14 Absent
PrachConfig15 Absent
PrachConfig16 Absent

Total Sccpch Config: 1
sttd_Indicator: FALSE
SccpchConfig 2 Absent
SccpchConfig 3 Absent
SccpchConfig 4 Absent
SccpchConfig 5 Absent
SccpchConfig 6 Absent
SccpchConfig 7 Absent
SccpchConfig 8 Absent
SccpchConfig 9 Absent
SccpchConfig 10 Absent
SccpchConfig 11 Absent
SccpchConfig 12 Absent
SccpchConfig 13 Absent
SccpchConfig 14 Absent
SccpchConfig 15 Absent
SccpchConfig 16 Absent

SIB 6 & 7 not present

SIB 11

Sib12Indicator: False
HCS Used: False
Quality Type: CPICH-ECNO
Intra-Frequency Cells: Present
Inter-Frequency Cells: Present
Inter-Rat Cells: Absent

Total Intra-Freq Cell: 30
Cell1 PSC: 124
Cell2 PSC: 189
Cell3 PSC: 163
Cell4 PSC: 262
Cell5 PSC: 384
Cell6 PSC: 373
Cell7 PSC: 333
Cell8 PSC: 287
Cell9 PSC: 303
Cell10 PSC: 326
Cell11 PSC: 192
Cell12 PSC: 372
Cell13 PSC: 338
Cell14 PSC: 376
Cell15 PSC: 149
Cell16 PSC: 39
Cell17 PSC: 184
Cell18 PSC: 398
Cell19 PSC: 375
Cell20 PSC: 300
Cell21 PSC: 135
Cell22 PSC: 218
Cell23 PSC: 474
Cell24 PSC: 429
Cell25 PSC: 332
Cell26 PSC: 346
Cell27 PSC: 364
Cell28 PSC: 288
Cell29 PSC: 480
Cell30 PSC: 231

Total Inter-Freq Cell: 1
Cell1 UARFCN: 10564 PSC: 184