MASTER INFORMATION BLOCK
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 20
  mib
    mib-ValueTag : 8
    plmn-Type
      gsm-MAP
        plmn-Identity
          mcc
            MCC[0]
              Digit : 2
            MCC[1]
              Digit : 2
            MCC[2]
              Digit : 6
          mnc
            MNC[0]
              Digit : 0
            MNC[1]
              Digit : 1
    sibSb-ReferenceList
      SIBSb-ReferenceList[0]
        sibSb-Type
          sysInfoTypeSB1 : 4
        scheduling
          scheduling
            sib-Pos
              rep8 : 1
      SIBSb-ReferenceList[1]
        sibSb-Type
          sysInfoType5 : 4
        scheduling
          scheduling
            segCount : 3
            sib-Pos
              rep32 : 2
            sib-PosOffsetInfo
              SibOFF-List[0]
                SibOFF : so2
              SibOFF-List[1]
                SibOFF : so6
      SIBSb-ReferenceList[2]
        sibSb-Type
        scheduling
          scheduling
            sib-Pos
              rep8 : 1
      SIBSb-ReferenceList[3]
        sibSb-Type
          sysInfoType11 : 2
        scheduling
          scheduling
            segCount : 9
            sib-Pos
              rep128 : 11
            sib-PosOffsetInfo
              SibOFF-List[0]
                SibOFF : so6
              SibOFF-List[1]
                SibOFF : so2
              SibOFF-List[2]
                SibOFF : so24
              SibOFF-List[3]
                SibOFF : so6
              SibOFF-List[4]
                SibOFF : so2
              SibOFF-List[5]
                SibOFF : so24
              SibOFF-List[6]
                SibOFF : so6
              SibOFF-List[7]
                SibOFF : so2

SYS.INFO.TYPE SB1
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 17
  sysInfoSB1
    sib-ReferenceList
      SIB-ReferenceList[0]
        sib-Type
          sysInfoType1 : 84
        scheduling
          scheduling
            sib-Pos
              rep64 : 7
      SIB-ReferenceList[1]
        sib-Type
          sysInfoType2 : 2
        scheduling
          scheduling
            sib-Pos
              rep32 : 6
      SIB-ReferenceList[2]
        sib-Type
          sysInfoType3 : 4
        scheduling
          scheduling
            sib-Pos
              rep64 : 26
      SIB-ReferenceList[3]
        sib-Type
          sysInfoType4 : 4
        scheduling
          scheduling
            sib-Pos
              rep128 : 23
    v6b0NonCriticalExtensions
      sysInfoTypeSB1-v6b0ext
      v860NonCriticalExtensions
        sysInfoTypeSB1-v860ext
          extSIBTypeInfoSchedulingInfo-List
            ExtSIBTypeInfoSchedulingInfo-List2[0]
              extensionSIB-Type2
              schedulingInfo
                scheduling
                  segCount : 2
                  sib-Pos
                    rep64 : 10
                  sib-PosOffsetInfo
                    SibOFF-List[0]
                      SibOFF : so32
              valueTagInfo
                cellValueTag : 2

SYS.INFO.TYPE 1
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 20
  sysInfoType1
    cn-CommonGSM-MAP-NAS-SysInfo : '3309'H (13065)
    cn-DomainSysInfoList
      CN-DomainSysInfoList[0]
        cn-DomainIdentity : cs-domain
        cn-Type
          gsm-MAP : '2801'H (10241)
        cn-DRX-CycleLengthCoeff : 7
      CN-DomainSysInfoList[1]
        cn-DomainIdentity : ps-domain
        cn-Type
          gsm-MAP : '0101'H (257)
        cn-DRX-CycleLengthCoeff : 7
    ue-ConnTimersAndConstants
      t-302 : ms3000
      n-304 : 3
      t-308 : ms40
      t-310 : ms40
      n-310 : 0
      t-311 : ms250
      t-312 : 6
      n-313 : s50
      t-315 : s30
      t-317 : infinity2
    ue-IdleTimersAndConstants
      t-300 : ms2000
      n-300 : 3
      t-312 : 6
      n-312 : s1
    v3a0NonCriticalExtensions
      sysInfoType1-v3a0ext
        ue-ConnTimersAndConstants-v3a0ext
        ue-IdleTimersAndConstants-v3a0ext
      v860NonCriticalExtentions
        sysInfoType1-v860ext
          ue-ConnTimersAndConstants
            t-323 : s5

SYS.INFO.TYPE 2
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 4
  sysInfoType2
    ura-IdentityList
      URA-IdentityList[0]
        URA-Identity : '3309'H (13065)

SYS.INFO.TYPE 3
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 19
  sysInfoType3
    sib4indicator : true
    cellIdentity : '51ADB04'H (85646084)
    cellSelectReselectInfo
      cellSelectQualityMeasure
        cpich-Ec-N0
          q-HYST-2-S : 1
      modeSpecificInfo
        fdd
          s-Intrasearch : 6
          s-Intersearch : 6
          rat-List
            RAT-FDD-InfoList[0]
              rat-Identifier : gsm
              s-SearchRAT : 1
              s-Limit-SearchRAT : 0
          q-QualMin : -18
          q-RxlevMin : -58
      q-Hyst-l-S : 2
      t-Reselection-S : 1
      maxAllowedUL-TX-Power : 24
    cellAccessRestriction
      cellBarred
      cellReservedForOperatorUse : notReserved
      cellReservationExtension : notReserved
      accessClassBarredList
        AccessClassBarredList[0]
          AccessClassBarred : notBarred
        AccessClassBarredList[1]
          AccessClassBarred : notBarred
        AccessClassBarredList[2]
          AccessClassBarred : notBarred
        AccessClassBarredList[3]
          AccessClassBarred : notBarred
        AccessClassBarredList[4]
          AccessClassBarred : notBarred
        AccessClassBarredList[5]
          AccessClassBarred : notBarred
        AccessClassBarredList[6]
          AccessClassBarred : notBarred
        AccessClassBarredList[7]
          AccessClassBarred : notBarred
        AccessClassBarredList[8]
          AccessClassBarred : notBarred
        AccessClassBarredList[9]
          AccessClassBarred : notBarred
        AccessClassBarredList[10]
          AccessClassBarred : notBarred
        AccessClassBarredList[11]
          AccessClassBarred : notBarred
        AccessClassBarredList[12]
          AccessClassBarred : notBarred
        AccessClassBarredList[13]
          AccessClassBarred : notBarred
        AccessClassBarredList[14]
          AccessClassBarred : notBarred
        AccessClassBarredList[15]
          AccessClassBarred : notBarred
    v4b0NonCriticalExtensions
      sysInfoType3-v4b0ext
      v590NonCriticalExtension
        sysInfoType3-v590ext
        v5c0NoncriticalExtension
          sysInfoType3-v5c0ext
          v670NonCriticalExtension
            sysInfoType3-v670ext
              domainSpecificAccessRestrictionParametersForPLMNOfMIB
                cSDomainSpecificAccessRestriction
                pSDomainSpecificAccessRestriction
            v770NonCriticalExtension
              sysInfoType3-v770ext
                deferredMeasurementControlReadingSupport
                  modeSpecificInfo
                    fdd
                      intraFreqMeasQuantity-FDD : cpich-Ec-N0

SYS.INFO.TYPE 4
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 16
  sysInfoType4
    cellIdentity : '51ADB04'H (85646084)
    cellSelectReselectInfo
      cellSelectQualityMeasure
        cpich-Ec-N0
          q-HYST-2-S : 1
      modeSpecificInfo
        fdd
          s-Intrasearch : 5
          s-Intersearch : 5
          rat-List
            RAT-FDD-InfoList[0]
              rat-Identifier : gsm
              s-SearchRAT : 1
              s-Limit-SearchRAT : 0
          q-QualMin : -18
          q-RxlevMin : -58
      q-Hyst-l-S : 2
      t-Reselection-S : 1
      maxAllowedUL-TX-Power : 24
    cellAccessRestriction
      cellBarred
      cellReservedForOperatorUse : notReserved
      cellReservationExtension : notReserved
      accessClassBarredList
        AccessClassBarredList[0]
          AccessClassBarred : notBarred
        AccessClassBarredList[1]
          AccessClassBarred : notBarred
        AccessClassBarredList[2]
          AccessClassBarred : notBarred
        AccessClassBarredList[3]
          AccessClassBarred : notBarred
        AccessClassBarredList[4]
          AccessClassBarred : notBarred
        AccessClassBarredList[5]
          AccessClassBarred : notBarred
        AccessClassBarredList[6]
          AccessClassBarred : notBarred
        AccessClassBarredList[7]
          AccessClassBarred : notBarred
        AccessClassBarredList[8]
          AccessClassBarred : notBarred
        AccessClassBarredList[9]
          AccessClassBarred : notBarred
        AccessClassBarredList[10]
          AccessClassBarred : notBarred
        AccessClassBarredList[11]
          AccessClassBarred : notBarred
        AccessClassBarredList[12]
          AccessClassBarred : notBarred
        AccessClassBarredList[13]
          AccessClassBarred : notBarred
        AccessClassBarredList[14]
          AccessClassBarred : notBarred
        AccessClassBarredList[15]
          AccessClassBarred : notBarred

SYS.INFO.TYPE 5
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 69
  sysInfoType5
    sib6indicator : false
    pich-PowerOffset : -7
    modeSpecificInfo
      fdd
        aich-PowerOffset : -6
    primaryCCPCH-Info
      fdd
        tx-DiversityIndicator : false
    prach-SystemInformationList
      PRACH-SystemInformationList[0]
        prach-RACH-Info
          modeSpecificInfo
            fdd
              availableSignatures : '00FF'H (255)
              availableSF : sfpr32
              preambleScramblingCodeWordNumber : 0
              puncturingLimit : pl1
              availableSubChannelNumbers : 'FFF'H (4095)
        transportChannelIdentity : 1
        rach-TransportFormatSet
          commonTransChTFS
            tti
              tti20
                CommonDynamicTF-InfoList[0]
                  rlc-Size
                    fdd
                      octetModeRLC-SizeInfoType2
                        sizeType1 : 15
                  numberOfTbSizeList[0]
                  logicalChannelList
                CommonDynamicTF-InfoList[1]
                  rlc-Size
                    fdd
                      octetModeRLC-SizeInfoType2
                        sizeType2 : 3
                  numberOfTbSizeList[0]
                  logicalChannelList
            semistaticTF-Information
              channelCodingType
                convolutional : half
              rateMatchingAttribute : 1
              crc-Size : crc16
        rach-TFCS
          normalTFCI-Signalling
            complete
              ctfcSize
                ctfc2Bit[0]
                  ctfc2 : 0
                  powerOffsetInformation
                    gainFactorInformation
                      signalledGainFactors
                        modeSpecificInfo
                          fdd
                            gainFactorBetaC : 13
                        gainFactorBetaD : 15
                    powerOffsetPp-m : -3
                ctfc2Bit[1]
                  ctfc2 : 1
                  powerOffsetInformation
                    gainFactorInformation
                      signalledGainFactors
                        modeSpecificInfo
                          fdd
                            gainFactorBetaC : 10
                        gainFactorBetaD : 15
                    powerOffsetPp-m : -2
        prach-Partitioning
          fdd[0]
            accessServiceClass-FDD
              availableSignatureStartIndex : 0
              availableSignatureEndIndex : 7
              assignedSubChannelNumber : 'F'H (15)
        ac-To-ASC-MappingTable
          AC-To-ASC-MappingTable[0]
            AC-To-ASC-Mapping : 0
          AC-To-ASC-MappingTable[1]
            AC-To-ASC-Mapping : 0
          AC-To-ASC-MappingTable[2]
            AC-To-ASC-Mapping : 0
          AC-To-ASC-MappingTable[3]
            AC-To-ASC-Mapping : 0
          AC-To-ASC-MappingTable[4]
            AC-To-ASC-Mapping : 0
          AC-To-ASC-MappingTable[5]
            AC-To-ASC-Mapping : 0
          AC-To-ASC-MappingTable[6]
            AC-To-ASC-Mapping : 0
        modeSpecificInfo
          fdd
            primaryCPICH-TX-Power : 35
            constantValue : -25
            prach-PowerOffset
              powerRampStep : 2
              preambleRetransMax : 15
            rach-TransmissionParameters
              mmax : 8
              nb01Min : 0
              nb01Max : 0
            aich-Info
              channelisationCode256 : 2
              sttd-Indicator : false
              aich-TransmissionTiming : e1
    sCCPCH-SystemInformationList
      SCCPCH-SystemInformationList[0]
        secondaryCCPCH-Info
          modeSpecificInfo
            fdd
              dummy1 : mayBeUsed
              sttd-Indicator : false
              sf-AndCodeNumber
                sf64 : 1
              pilotSymbolExistence : false
              tfci-Existence : true
              positionFixedOrFlexible : flexible
              timingOffset : 50
        tfcs
          normalTFCI-Signalling
            complete
              ctfcSize
                ctfc4Bit[0]
                  ctfc4 : 0
                ctfc4Bit[1]
                  ctfc4 : 1
                ctfc4Bit[2]
                  ctfc4 : 2
                ctfc4Bit[3]
                  ctfc4 : 3
                ctfc4Bit[4]
                  ctfc4 : 4
                ctfc4Bit[5]
                  ctfc4 : 6
        fach-PCH-InformationList
          FACH-PCH-InformationList[0]
            transportFormatSet
              commonTransChTFS
                tti
                  tti10
                    CommonDynamicTF-InfoList[0]
                      rlc-Size
                        fdd
                          octetModeRLC-SizeInfoType2
                            sizeType1 : 24
                      numberOfTbSizeList[0]
                      numberOfTbSizeList[1]
                      logicalChannelList
                semistaticTF-Information
                  channelCodingType
                    convolutional : half
                  rateMatchingAttribute : 230
                  crc-Size : crc16
            transportChannelIdentity : 3
            ctch-Indicator : false
          FACH-PCH-InformationList[1]
            transportFormatSet
              commonTransChTFS
                tti
                  tti10
                    CommonDynamicTF-InfoList[0]
                      rlc-Size
                        fdd
                          octetModeRLC-SizeInfoType2
                            sizeType1 : 15
                      numberOfTbSizeList[0]
                      numberOfTbSizeList[1]
                      numberOfTbSizeList[2]
                        small : 2
                      logicalChannelList
                semistaticTF-Information
                  channelCodingType
                    convolutional : half
                  rateMatchingAttribute : 220
                  crc-Size : crc16
            transportChannelIdentity : 4
            ctch-Indicator : false
          FACH-PCH-InformationList[2]
            transportFormatSet
              commonTransChTFS
                tti
                  tti10
                    CommonDynamicTF-InfoList[0]
                      rlc-Size
                        fdd
                          octetModeRLC-SizeInfoType2
                            sizeType2 : 3
                      numberOfTbSizeList[0]
                      numberOfTbSizeList[1]
                      logicalChannelList
                semistaticTF-Information
                  channelCodingType
                  rateMatchingAttribute : 130
                  crc-Size : crc16
            transportChannelIdentity : 5
            ctch-Indicator : false
        pich-Info
          fdd
            channelisationCode256 : 3
            pi-CountPerFrame : e36
            sttd-Indicator : false
    v4b0NonCriticalExtensions
      sysInfoType5-v4b0ext
        frequencyBandIndicator : fdd2100
      v590NonCriticalExtensions
        v650NonCriticalExtensions
          v680NonCriticalExtensions
            sysInfoType5-v680ext
              hsdpa-CellIndicator : hsdpa-CapableCell
            v690NonCriticalExtensions
              sysInfoType5-v690ext
                edch-CellIndicator : edch-CapableCell

SYS.INFO.TYPE 7
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 4
  sysInfoType7
    modeSpecificInfo
      fdd
        ul-Interference : -105
    prach-Information-SIB5-List
      DynamicPersistenceLevelList[0]
        DynamicPersistenceLevel : 1

SYS.INFO.TYPE 11
WCDMA RRC Signaling Messages
  Channel Type : UnKnOwN (254)
  RB ID : 40
  Length : 238
  sysInfoType11
    sib12indicator : false
    fach-MeasurementOccasionInfo
      fACH-meas-occasion-coeff : 3
      inter-freq-FDD-meas-ind : true
      inter-freq-TDD-meas-ind : false
      inter-RAT-meas-ind[0]
        RAT-Type : gsm
    measurementControlSysInfo
      use-of-HCS
        hcs-not-used
          cellSelectQualityMeasure
            cpich-Ec-N0
              intraFreqMeasurementSysInfo
                intraFreqCellInfoSI-List
                  removedIntraFreqCellList
                  newIntraFreqCellList
                    NewIntraFreqCellSI-List-ECN0[0]
                      intraFreqCellID : 0
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 73
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[1]
                      intraFreqCellID : 1
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 322
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[2]
                      intraFreqCellID : 2
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 54
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[3]
                      intraFreqCellID : 3
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 475
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[4]
                      intraFreqCellID : 4
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 107
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[5]
                      intraFreqCellID : 5
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 39
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[6]
                      intraFreqCellID : 6
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 130
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[7]
                      intraFreqCellID : 7
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 53
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[8]
                      intraFreqCellID : 8
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 359
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[9]
                      intraFreqCellID : 9
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 409
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[10]
                      intraFreqCellID : 10
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 167
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[11]
                      intraFreqCellID : 11
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 229
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[12]
                      intraFreqCellID : 12
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 59
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[13]
                      intraFreqCellID : 13
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 419
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[14]
                      intraFreqCellID : 14
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 307
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[15]
                      intraFreqCellID : 15
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 461
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[16]
                      intraFreqCellID : 16
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 115
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[17]
                      intraFreqCellID : 17
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 371
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewIntraFreqCellSI-List-ECN0[18]
                      intraFreqCellID : 18
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 247
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false

                intraFreqReportingQuantityForRACH
                  sfn-SFN-OTD-Type : noReport
                  modeSpecificInfo
                    fdd
                      intraFreqRepQuantityRACH-FDD : cpich-EcN0
                maxReportedCellsOnRACH : currentAnd-2-BestNeighbour
              interFreqMeasurementSysInfo
                interFreqCellInfoSI-List
                  removedInterFreqCellList
                  newInterFreqCellList
                    NewInterFreqCellSI-List-ECN0[0]
                      interFreqCellID : 0
                      frequencyInfo
                        modeSpecificInfo
                          fdd
                            uarfcn-UL : 2713
                            uarfcn-DL : 2938
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 73
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[1]
                      interFreqCellID : 1
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 59
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[2]
                      interFreqCellID : 2
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 12
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[3]
                      interFreqCellID : 3
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 499
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[4]
                      interFreqCellID : 4
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 362
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[5]
                      interFreqCellID : 5
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 419
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[6]
                      interFreqCellID : 6
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 440
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[7]
                      interFreqCellID : 7
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 30
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[8]
                      interFreqCellID : 8
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 292
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[9]
                      interFreqCellID : 9
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 409
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[10]
                      interFreqCellID : 10
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 167
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[11]
                      interFreqCellID : 11
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 130
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[12]
                      interFreqCellID : 12
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 39
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[13]
                      interFreqCellID : 13
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 359
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[14]
                      interFreqCellID : 14
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 53
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[15]
                      interFreqCellID : 15
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 196
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[16]
                      interFreqCellID : 16
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 382
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[17]
                      interFreqCellID : 17
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 475
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[18]
                      interFreqCellID : 18
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 107
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[19]
                      interFreqCellID : 19
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 488
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[20]
                      interFreqCellID : 20
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 183
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[21]
                      interFreqCellID : 21
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 115
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false
                    NewInterFreqCellSI-List-ECN0[22]
                      interFreqCellID : 22
                      cellInfo
                        modeSpecificInfo
                          fdd
                            primaryCPICH-Info
                              primaryScramblingCode : 307
                            readSFN-Indicator : true
                            tx-DiversityIndicator : false

          interRATMeasurementSysInfo
            nterRATCellInfoList
              removedInterRATCellList
              newInterRATCellList
                NewInterRATCellList-B[0]
                  interRATCellID : 0
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 0
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -50
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 5
                        bcc : 5
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 1013
                NewInterRATCellList-B[1]
                  interRATCellID : 1
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 0
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -50
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 0
                        bcc : 0
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 1017
                NewInterRATCellList-B[2]
                  interRATCellID : 2
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 0
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -50
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 5
                        bcc : 5
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 1022
                NewInterRATCellList-B[3]
                  interRATCellID : 3
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 0
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -50
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 5
                        bcc : 0
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 1015
                NewInterRATCellList-B[4]
                  interRATCellID : 4
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 0
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -50
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 4
                        bcc : 6
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 1023
                NewInterRATCellList-B[5]
                  interRATCellID : 5
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 0
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -50
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 5
                        bcc : 1
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 1016
                NewInterRATCellList-B[6]
                  interRATCellID : 6
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 0
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -50
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 5
                        bcc : 2
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 1019
                NewInterRATCellList-B[7]
                  interRATCellID : 7
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 0
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -50
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 5
                        bcc : 4
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 1013
                NewInterRATCellList-B[8]
                  interRATCellID : 8
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 0
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -50
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 4
                        bcc : 1
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 1020
                NewInterRATCellList-B[9]
                  interRATCellID : 9
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 0
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -50
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 5
                        bcc : 5
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 1020
                NewInterRATCellList-B[10]
                  interRATCellID : 10
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 0
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -50
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 4
                        bcc : 7
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 1015
                NewInterRATCellList-B[11]
                  interRATCellID : 11
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 0
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -50
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 4
                        bcc : 7
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 1022
                NewInterRATCellList-B[12]
                  interRATCellID : 12
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 0
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -50
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 5
                        bcc : 1
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 1021
                NewInterRATCellList-B[13]
                  interRATCellID : 13
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 0
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -50
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 0
                        bcc : 1
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 1022
                NewInterRATCellList-B[14]
                  interRATCellID : 14
                  technologySpecificInfo
                    gsm
                      cellSelectionReselectionInfo
                        q-Offset1S-N : 0
                        modeSpecificInfo
                          gsm
                            q-RxlevMin : -50
                      interRATCellIndividualOffset : 0
                      bsic
                        ncc : 4
                        bcc : 7
                      frequency-band : dcs1800BandUsed
                      bcch-ARFCN : 1018

No SYS.INFO.TYPE 19

————————————————————————————————
BlackBerry 9720
————————————————————————————————

CELL INFORMATION

3G CS+PS PDP CELL_PCH
RRC State: CELL_PCH

PSC=73 UARFCN=(1)10836 RSSI=-71
MCC: 226  MNC:1f LAC: 3309 RAC:0001
NCO: 0  NMO: 1
MSC Rev: 99+ SGSN Rev: 99+

URA_ID: later
DRX Cycle Length: 64

SIB VALIDITY

Uarfcn = 10836 and Psc = 73
MIB validity = Valid
SIB1 validity = Valid
SIB2 validity = Valid
SIB3 validity = Valid
SIB4 validity = Valid
SIB5 validity = Valid
SIB6 validity = Invalid
SIB7 validity = Invalid
SIB11 validity = Valid
SIB12 validity = Invalid
SIB13 validity = Invalid
SIB13.1 validity = Invalid
SIB13.2 validity = Invalid
SIB13.3 validity = Invalid
SIB13.4 validity = Invalid
SIB14 validity = Invalid
SIB15 validity = Invalid
SIB15.1 validity = Invalid
SIB15.2 validity = Invalid
SIB15.3 validity = Invalid
SIB16 validity = Invalid
SIB17 validity = Invalid
SIB15.4 validity = Invalid
SIB18 validity = Invalid
SB1 validity = Valid
SB2 validity = Invalid
SIB15.5 validity = Invalid

MIB

MIB Value Tag: 8
MCC:2 2 6  MNC:0  d 1 
SIB1 not scheduled in MIB
SIB2 not scheduled in MIB
SIB3 not scheduled in MIB
SIB4 not scheduled in MIB
SIB5 scheduled with tag 4
SIB6 not scheduled in MIB
SIB7 scheduled with tag 0
SIB11 scheduled with tag 2
SIB12 not scheduled in MIB
SIB13 not scheduled in MIB
SIB13.1 not scheduled in MIB
SIB13.2 not scheduled in MIB
SIB13.3 not scheduled in MIB
SIB13.4 not scheduled in MIB
SIB14 not scheduled in MIB
SIB15 not scheduled in MIB
SIB16 not scheduled in MIB
SIB17 not scheduled in MIB
SB1 scheduled with tag 4
SB2 not scheduled in MIB
SIB15.1 not scheduled in MIB
SIB15.2 not scheduled in MIB
SIB15.2 not scheduled in MIB
SIB15.4 not scheduled in MIB
SIB18 not scheduled in MIB
SIB15.5 not scheduled in MIB

SCHEDULING BLK 1

SIB1 scheduled with tag 84
SIB2 scheduled with tag 2
SIB3 scheduled with tag 4
SIB4 scheduled with tag 4
SIB5 not scheduled in sb1
SIB6 not scheduled in sb1
SIB7 not scheduled in sb1
SIB11 not scheduled in sb1
SIB12 not scheduled in sb1
SIB13 not scheduled in sb1
SIB13.1 not scheduled in sb1
SIB13.2 not scheduled in sb1
SIB13.3 not scheduled in sb1
SIB13.4 not scheduled in sb1
SIB14 not scheduled in sb1
SIB15 not scheduled in sb1
SIB16 not scheduled in sb1
SIB17 not scheduled in sb1
SB1 not scheduled in sb1
sb1 not scheduled in sb1
SIB15.1 not scheduled in sb1
SIB15.2 not scheduled in sb1
SIB15.2 not scheduled in sb1
SIB15.4 not scheduled in sb1
SIB18 not scheduled in sb1
SIB15.5 not scheduled in sb1

SB 2 not present

SIB 1

T300: 2000
N300: 3
T302: 3000
N302: 3
T323: 5

SIB 2

Number of UraId: 1
UraId1 = 13065:
UraId2 Absent
UraId3 Absent
UraId4 Absent
UraId5 Absent
UraId6 Absent
UraId7 Absent
UraId8 Absent

SIB 3

Cell Identity: 85646084
Sib4Indicator: True
Barred Status: Not Barred
Reserve Indicator: Not reserved
Access Barred list: Present
AccessBarredClassBitmap: 0
Cell Sel Critieria: CPICH-Ec/No
Qqualmin: -18
QrxlevMin: -58
Max UL TX Power: 24
s_IntraSearch: 12
s_InterSearch: 12
s_SearchHCS: INVALID
s_HCS_GSM: INVALID
s_Limit_SearchRAT: 0

SIB 4

Cell Identity: 85646084
Barred Status: Not Barred
Reserve Indicator: Not reserved
Access Barred list is Present
AccessBarredClassBitmap: 0
Cell sel critieria is: CPICH-Ec/No
Qqualmin value: -18
QrxlevMin value: -58
Max UL TX power: 24
s_IntraSearch: 10
s_InterSearch: 10
s_SearchHCS: INVALID
s_HCS_GSM: INVALID
s_Limit_SearchRAT: 0

SIB 5

Sib6Indicator: False
Total Prach Config: 1
Step:2 RetranMax:15 mMax:8
PrachConfig2 Absent
PrachConfig3 Absent
PrachConfig4 Absent
PrachConfig5 Absent
PrachConfig6 Absent
PrachConfig7 Absent
PrachConfig8 Absent
PrachConfig9 Absent
PrachConfig10 Absent
PrachConfig11 Absent
PrachConfig12 Absent
PrachConfig13 Absent
PrachConfig14 Absent
PrachConfig15 Absent
PrachConfig16 Absent

Total Sccpch Config: 1
sttd_Indicator: FALSE
SccpchConfig 2 Absent
SccpchConfig 3 Absent
SccpchConfig 4 Absent
SccpchConfig 5 Absent
SccpchConfig 6 Absent
SccpchConfig 7 Absent
SccpchConfig 8 Absent
SccpchConfig 9 Absent
SccpchConfig 10 Absent
SccpchConfig 11 Absent
SccpchConfig 12 Absent
SccpchConfig 13 Absent
SccpchConfig 14 Absent
SccpchConfig 15 Absent
SccpchConfig 16 Absent

SIB 6 & 7 not present

SIB 11

Sib12Indicator: False
HCS Used: False
Quality Type: CPICH-ECNO
Intra-Frequency Cells: Present
Inter-Frequency Cells: Present
Inter-Rat Cells: Present

Total Intra-Freq Cell: 19
Cell1 PSC: 73
Cell2 PSC: 322
Cell3 PSC: 54
Cell4 PSC: 475
Cell5 PSC: 107
Cell6 PSC: 39
Cell7 PSC: 130
Cell8 PSC: 53
Cell9 PSC: 359
Cell10 PSC: 409
Cell11 PSC: 167
Cell12 PSC: 229
Cell13 PSC: 59
Cell14 PSC: 419
Cell15 PSC: 307
Cell16 PSC: 461
Cell17 PSC: 115
Cell18 PSC: 371
Cell19 PSC: 247

Total Inter-Freq Cell: 1
Cell1 UARFCN: 2938 PSC: 73

Total Inter-RAT Cell: 15
Cell1 Band:DCS1800 ARFCN:1013 BSIC:5 5
Cell2 Band:DCS1800 ARFCN:1017 BSIC:0 0
Cell3 Band:DCS1800 ARFCN:1022 BSIC:5 5
Cell4 Band:DCS1800 ARFCN:1015 BSIC:5 0
Cell5 Band:DCS1800 ARFCN:1023 BSIC:4 6
Cell6 Band:DCS1800 ARFCN:1016 BSIC:5 1
Cell7 Band:DCS1800 ARFCN:1019 BSIC:5 2
Cell8 Band:DCS1800 ARFCN:1013 BSIC:5 4
Cell9 Band:DCS1800 ARFCN:1020 BSIC:4 1
Cell10 Band:DCS1800 ARFCN:1020 BSIC:5 5
Cell11 Band:DCS1800 ARFCN:1015 BSIC:4 7
Cell12 Band:DCS1800 ARFCN:1022 BSIC:4 7
Cell13 Band:DCS1800 ARFCN:1021 BSIC:5 1
Cell14 Band:DCS1800 ARFCN:1022 BSIC:0 1
Cell15 Band:DCS1800 ARFCN:1018 BSIC:4 7

NEIGHBOUR CELLS

Active RAT is UTRAN - CELL_PCH

IntraFreqCells 19 Uarfcn:10836 RSSI:-79
S PSC:73 EcNo:-11 RSCP:-91
 PSC:322 EcNo:-40 RSCP:-167
 PSC:54 EcNo:-40 RSCP:-167
 PSC:475 EcNo:-40 RSCP:-167
 PSC:107 EcNo:-40 RSCP:-167
 PSC:39 EcNo:-40 RSCP:-167
 PSC:130 EcNo:-40 RSCP:-167
 PSC:53 EcNo:-40 RSCP:-167
 PSC:359 EcNo:-40 RSCP:-167
 PSC:409 EcNo:-40 RSCP:-167
 PSC:167 EcNo:-40 RSCP:-167
 PSC:229 EcNo:-40 RSCP:-167
 PSC:59 EcNo:-40 RSCP:-167
 PSC:419 EcNo:-40 RSCP:-167
 PSC:307 EcNo:-40 RSCP:-167
 PSC:461 EcNo:-40 RSCP:-167
 PSC:115 EcNo:-40 RSCP:-167
 PSC:371 EcNo:-40 RSCP:-167
 PSC:247 EcNo:-40 RSCP:-167

InterFreq Cells : 23
Uarfcn: 2938 RSSI: -64
PSC:73 EcNo:-13 RSCP:-77
PSC:59 EcNo:-40 RSCP:-167
PSC:12 EcNo:-40 RSCP:-167
PSC:499 EcNo:-40 RSCP:-167
PSC:362 EcNo:-40 RSCP:-167
PSC:419 EcNo:-40 RSCP:-167
PSC:440 EcNo:-40 RSCP:-167
PSC:30 EcNo:-40 RSCP:-167
PSC:292 EcNo:-40 RSCP:-167
PSC:409 EcNo:-40 RSCP:-167
PSC:167 EcNo:-40 RSCP:-167
PSC:130 EcNo:-40 RSCP:-167
PSC:39 EcNo:-40 RSCP:-167
PSC:359 EcNo:-40 RSCP:-167
PSC:53 EcNo:-40 RSCP:-167
PSC:196 EcNo:-40 RSCP:-167
PSC:382 EcNo:-40 RSCP:-167
PSC:475 EcNo:-40 RSCP:-167
PSC:107 EcNo:-40 RSCP:-167
PSC:488 EcNo:-40 RSCP:-167
PSC:183 EcNo:-40 RSCP:-167
PSC:115 EcNo:-40 RSCP:-167
PSC:307 EcNo:-40 RSCP:-167